From 9d152df885cb6f6874259d93df558e649f62774f Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Fri, 25 Jun 2010 16:01:00 -0500
Subject: [PATCH 28/75] omap3beagle: camera: Set padconf settings in cam init

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 arch/arm/mach-omap2/board-omap3beagle-camera.c |   35 ++++++++++++++++++++++++
 1 files changed, 35 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle-camera.c b/arch/arm/mach-omap2/board-omap3beagle-camera.c
index b0148d6..75471f2 100644
--- a/arch/arm/mach-omap2/board-omap3beagle-camera.c
+++ b/arch/arm/mach-omap2/board-omap3beagle-camera.c
@@ -34,6 +34,7 @@
 
 #include <plat/mux.h>
 #include <plat/board.h>
+#include <plat/control.h>
 
 #include <media/v4l2-int-device.h>
 #include <media/mt9t111.h>
@@ -285,6 +286,40 @@ static int beagle_cam_remove(struct platform_device *pdev)
 
 	gpio_free(LEOPARD_RESET_GPIO);
 
+	/* MUX init */
+	omap_ctrl_writew(OMAP_PIN_INPUT_PULLUP | OMAP_MUX_MODE0,
+			 0x10C); /* CAM_HS */
+	omap_ctrl_writew(OMAP_PIN_INPUT_PULLUP | OMAP_MUX_MODE0,
+			 0x10E); /* CAM_VS */
+	omap_ctrl_writew(OMAP_PIN_OUTPUT | OMAP_MUX_MODE0,
+			 0x110); /* CAM_XCLKA */
+	omap_ctrl_writew(OMAP_PIN_INPUT_PULLUP | OMAP_MUX_MODE0,
+			 0x112); /* CAM_PCLK */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x116); /* CAM_D0 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x118); /* CAM_D1 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x11A); /* CAM_D2 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x11C); /* CAM_D3 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x11E); /* CAM_D4 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x120); /* CAM_D5 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x122); /* CAM_D6 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x124); /* CAM_D7 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x126); /* CAM_D8 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x128); /* CAM_D9 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x12A); /* CAM_D10 */
+	omap_ctrl_writew(OMAP_PIN_INPUT | OMAP_MUX_MODE0,
+			 0x12C); /* CAM_D11 */
+
 	return 0;
 }
 
-- 
1.6.6.1

