From f8c07cb92ea86609586270f60474814fc09da890 Mon Sep 17 00:00:00 2001
From: Sekhar Nori <nsekhar@ti.com>
Date: Wed, 28 Dec 2011 12:02:57 +0530
Subject: [PATCH 62/90] usb: musb: davinci: fix build breakage

commit 006896fc612f11bf0624db7814a75d0d5410855f upstream.

Commit 0020afb369859472a461ef4af6410732e929d402 (ARM: mach-davinci:
remove mach/memory.h) removed mach/memory.h for DaVinci which broke
DaVinci MUSB build.

mach/memory.h is not actually needed in davinci.c, so remove it.
While at it, also remove some more machine specific inclulde
files which are not needed for build.

Tested on DM644x EVM using USB card reader.

Signed-off-by: Sekhar Nori <nsekhar@ti.com>
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/musb/davinci.c |    3 ---
 1 file changed, 3 deletions(-)

diff --git a/drivers/usb/musb/davinci.c b/drivers/usb/musb/davinci.c
index 4d365d5..3911d9a 100644
--- a/drivers/usb/musb/davinci.c
+++ b/drivers/usb/musb/davinci.c
@@ -33,9 +33,6 @@
 #include <linux/platform_device.h>
 #include <linux/dma-mapping.h>
 
-#include <mach/hardware.h>
-#include <mach/memory.h>
-#include <asm/gpio.h>
 #include <mach/cputype.h>
 
 #include <asm/mach-types.h>
-- 
1.7.9.4

