From a3e4bd3ab18fd8f60692869405d89513fa7caecc Mon Sep 17 00:00:00 2001
From: Benjamin Tissoires <benjamin.tissoires@gmail.com>
Date: Fri, 23 Dec 2011 15:41:00 +0100
Subject: [PATCH 087/130] HID: multitouch: add support for 3M 32"

commit c4fad877cd0efb51d8180ae2eaa791c99c92051c upstream.

Signed-off-by: Benjamin Tissoires <benjamin.tissoires@gmail.com>
Acked-by: Henrik Rydberg <rydberg@euromail.se>
Signed-off-by: Jiri Kosina <jkosina@suse.cz>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/hid/hid-ids.h        |    1 +
 drivers/hid/hid-multitouch.c |    3 +++
 2 files changed, 4 insertions(+)

diff --git a/drivers/hid/hid-ids.h b/drivers/hid/hid-ids.h
index bf95a50..6e53391a 100644
--- a/drivers/hid/hid-ids.h
+++ b/drivers/hid/hid-ids.h
@@ -21,6 +21,7 @@
 #define USB_VENDOR_ID_3M		0x0596
 #define USB_DEVICE_ID_3M1968		0x0500
 #define USB_DEVICE_ID_3M2256		0x0502
+#define USB_DEVICE_ID_3M3266		0x0506
 
 #define USB_VENDOR_ID_A4TECH		0x09da
 #define USB_DEVICE_ID_A4TECH_WCP32PU	0x0006
diff --git a/drivers/hid/hid-multitouch.c b/drivers/hid/hid-multitouch.c
index 7f83024..4a63dee 100644
--- a/drivers/hid/hid-multitouch.c
+++ b/drivers/hid/hid-multitouch.c
@@ -609,6 +609,9 @@ static const struct hid_device_id mt_devices[] = {
 	{ .driver_data = MT_CLS_3M,
 		HID_USB_DEVICE(USB_VENDOR_ID_3M,
 			USB_DEVICE_ID_3M2256) },
+	{ .driver_data = MT_CLS_3M,
+		HID_USB_DEVICE(USB_VENDOR_ID_3M,
+			USB_DEVICE_ID_3M3266) },
 
 	/* ActionStar panels */
 	{ .driver_data = MT_CLS_DEFAULT,
-- 
1.7.9.4

