From 460ac29a1ee0577d6b9044caa53761cc0d02b495 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 25 Jan 2012 15:48:36 +0100
Subject: [PATCH 07/13] beagleboard: reinstate usage of hi-speed PLL divider

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    5 +++++
 1 files changed, 5 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index a546c2b..e28ae72 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -308,6 +308,11 @@ static struct omap_dss_device beagle_dvi_device = {
 	.driver_name = "dvi",
 	.data = &dvi_panel,
 	.phy.dpi.data_lines = 24,
+	.clocks = {
+		.dispc = {
+			.dispc_fclk_src = OMAP_DSS_CLK_SRC_DSI_PLL_HSDIV_DISPC,
+		},
+	},
 	.reset_gpio = -EINVAL,
 };
 
-- 
1.7.7.4

