From 2bb2e47c60f77b768affa48bf847526054143d81 Mon Sep 17 00:00:00 2001
From: Chris Wilson <chris@chris-wilson.co.uk>
Date: Thu, 22 Mar 2012 15:00:50 +0000
Subject: [PATCH 28/60] drm/i915: Sanitize BIOS debugging bits from PIPECONF

commit f47166d2b0001fcb752b40c5a2d4db986dfbea68 upstream.

Quoting the BSpec from time immemorial:

  PIPEACONF, bits 28:27: Frame Start Delay (Debug)

  Used to delay the frame start signal that is sent to the display planes.
  Care must be taken to insure that there are enough lines during VBLANK
  to support this setting.

An instance of the BIOS leaving these bits set was found in the wild,
where it caused our modesetting to go all squiffy and skewiff.

Bugzilla: https://bugs.freedesktop.org/show_bug.cgi?id=47271
Reported-and-tested-by: Eva Wang <evawang@linpus.com>
Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=43012
Reported-and-tested-by: Carl Richell <carl@system76.com>
Signed-off-by: Chris Wilson <chris@chris-wilson.co.uk>
Signed-off-by: Daniel Vetter <daniel.vetter@ffwll.ch>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/i915/i915_reg.h      |    1 +
 drivers/gpu/drm/i915/intel_display.c |    6 ++++++
 2 files changed, 7 insertions(+)

diff --git a/drivers/gpu/drm/i915/i915_reg.h b/drivers/gpu/drm/i915/i915_reg.h
index 1608d2a..2f99fd4 100644
--- a/drivers/gpu/drm/i915/i915_reg.h
+++ b/drivers/gpu/drm/i915/i915_reg.h
@@ -2312,6 +2312,7 @@
 #define   PIPECONF_DISABLE	0
 #define   PIPECONF_DOUBLE_WIDE	(1<<30)
 #define   I965_PIPECONF_ACTIVE	(1<<30)
+#define   PIPECONF_FRAME_START_DELAY_MASK (3<<27)
 #define   PIPECONF_SINGLE_WIDE	0
 #define   PIPECONF_PIPE_UNLOCKED 0
 #define   PIPECONF_PIPE_LOCKED	(1<<25)
diff --git a/drivers/gpu/drm/i915/intel_display.c b/drivers/gpu/drm/i915/intel_display.c
index 9ec9755..9011f48 100644
--- a/drivers/gpu/drm/i915/intel_display.c
+++ b/drivers/gpu/drm/i915/intel_display.c
@@ -7278,6 +7278,12 @@ static void intel_sanitize_modesetting(struct drm_device *dev,
 	struct drm_i915_private *dev_priv = dev->dev_private;
 	u32 reg, val;
 
+	/* Clear any frame start delays used for debugging left by the BIOS */
+	for_each_pipe(pipe) {
+		reg = PIPECONF(pipe);
+		I915_WRITE(reg, I915_READ(reg) & ~PIPECONF_FRAME_START_DELAY_MASK);
+	}
+
 	if (HAS_PCH_SPLIT(dev))
 		return;
 
-- 
1.7.9.5

