From e108118265e60d28d2aec2f4110c34cba5dfc86f Mon Sep 17 00:00:00 2001
From: Guenter Roeck <linux@roeck-us.net>
Date: Fri, 27 Jan 2012 05:43:59 -0800
Subject: [PATCH 48/87] hwmon: (w83627ehf) Fix number of fans for NCT6776F

commit 585c0fd8216e0c9f98e2434092af7ec0f999522d upstream.

NCT6776F can select fan input pins for fans 3 to 5 with a secondary set of
chip register bits. Check that second set of bits in addition to the first set
to detect if fans 3..5 are monitored.

Signed-off-by: Guenter Roeck <linux@roeck-us.net>
Acked-by: Jean Delvare <khali@linux-fr.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/hwmon/w83627ehf.c |   23 ++++++++++++++++++++---
 1 file changed, 20 insertions(+), 3 deletions(-)

diff --git a/drivers/hwmon/w83627ehf.c b/drivers/hwmon/w83627ehf.c
index 4b57ab6..c25387d 100644
--- a/drivers/hwmon/w83627ehf.c
+++ b/drivers/hwmon/w83627ehf.c
@@ -1920,9 +1920,26 @@ w83627ehf_check_fan_inputs(const struct w83627ehf_sio_data *sio_data,
 		fan4min = 0;
 		fan5pin = 0;
 	} else if (sio_data->kind == nct6776) {
-		fan3pin = !(superio_inb(sio_data->sioreg, 0x24) & 0x40);
-		fan4pin = !!(superio_inb(sio_data->sioreg, 0x1C) & 0x01);
-		fan5pin = !!(superio_inb(sio_data->sioreg, 0x1C) & 0x02);
+		bool gpok = superio_inb(sio_data->sioreg, 0x27) & 0x80;
+
+		superio_select(sio_data->sioreg, W83627EHF_LD_HWM);
+		regval = superio_inb(sio_data->sioreg, SIO_REG_ENABLE);
+
+		if (regval & 0x80)
+			fan3pin = gpok;
+		else
+			fan3pin = !(superio_inb(sio_data->sioreg, 0x24) & 0x40);
+
+		if (regval & 0x40)
+			fan4pin = gpok;
+		else
+			fan4pin = !!(superio_inb(sio_data->sioreg, 0x1C) & 0x01);
+
+		if (regval & 0x20)
+			fan5pin = gpok;
+		else
+			fan5pin = !!(superio_inb(sio_data->sioreg, 0x1C) & 0x02);
+
 		fan4min = fan4pin;
 	} else if (sio_data->kind == w83667hg || sio_data->kind == w83667hg_b) {
 		fan3pin = 1;
-- 
1.7.9.4

