From 08d76bb3139d89b31bbf05f2a4b279a739b47404 Mon Sep 17 00:00:00 2001
From: Roland Stigge <stigge@antcom.de>
Date: Mon, 27 Feb 2012 17:28:03 +0100
Subject: [PATCH 06/95] ARM: LPC32xx: serial.c: Fixed loop limit

commit ff424aa4c89d19082e8ae5a3351006bc8a4cd91b upstream.

This patch fixes a wrong loop limit on UART init.

Signed-off-by: Roland Stigge <stigge@antcom.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 arch/arm/mach-lpc32xx/serial.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/mach-lpc32xx/serial.c b/arch/arm/mach-lpc32xx/serial.c
index 1a3fd4c..f273528 100644
--- a/arch/arm/mach-lpc32xx/serial.c
+++ b/arch/arm/mach-lpc32xx/serial.c
@@ -187,7 +187,7 @@ void __init lpc32xx_serial_init(void)
 
 	/* This needs to be done after all UART clocks are setup */
 	__raw_writel(clkmodes, LPC32XX_UARTCTL_CLKMODE);
-	for (i = 0; i < ARRAY_SIZE(uartinit_data) - 1; i++) {
+	for (i = 0; i < ARRAY_SIZE(uartinit_data); i++) {
 		/* Force a flush of the RX FIFOs to work around a HW bug */
 		puart = serial_std_platform_data[i].mapbase;
 		__raw_writel(0xC1, LPC32XX_UART_IIR_FCR(puart));
-- 
1.7.9.4

