From 9db1b1f07b5ebad591e145671313720d4728d2d1 Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Wed, 22 Feb 2012 17:02:38 +0100
Subject: [PATCH 13/72] ALSA: hda - Fix redundant jack creations for cx5051

[Note that since the patch isn't applicable (and unnecessary) to
3.3-rc, there is no corresponding upstream fix.]

The cx5051 parser calls snd_hda_input_jack_add() in the init callback
to create and initialize the jack detection instances.  Since the init
callback is called at each time when the device gets woken up after
suspend or power-saving mode, the duplicated instances are accumulated
at each call.  This ends up with the kernel warnings with the too
large array size.

The fix is simply to move the calls of snd_hda_input_jack_add() into
the parser section instead of the init callback.

The fix is needed only up to 3.2 kernel, since the HD-audio jack layer
was redesigned in the 3.3 kernel.

Reported-by: Russell King <rmk+kernel@arm.linux.org.uk>
Tested-by: Russell King <rmk+kernel@arm.linux.org.uk>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/pci/hda/patch_conexant.c |   11 ++++++++++-
 1 file changed, 10 insertions(+), 1 deletion(-)

diff --git a/sound/pci/hda/patch_conexant.c b/sound/pci/hda/patch_conexant.c
index 7072251..08bad5b 100644
--- a/sound/pci/hda/patch_conexant.c
+++ b/sound/pci/hda/patch_conexant.c
@@ -1899,6 +1899,10 @@ static void cxt5051_init_mic_port(struct hda_codec *codec, hda_nid_t nid,
 	snd_hda_codec_write(codec, nid, 0,
 			    AC_VERB_SET_UNSOLICITED_ENABLE,
 			    AC_USRSP_EN | event);
+}
+
+static void cxt5051_init_mic_jack(struct hda_codec *codec, hda_nid_t nid)
+{
 	snd_hda_input_jack_add(codec, nid, SND_JACK_MICROPHONE, NULL);
 	snd_hda_input_jack_report(codec, nid);
 }
@@ -1916,7 +1920,6 @@ static int cxt5051_init(struct hda_codec *codec)
 	struct conexant_spec *spec = codec->spec;
 
 	conexant_init(codec);
-	conexant_init_jacks(codec);
 
 	if (spec->auto_mic & AUTO_MIC_PORTB)
 		cxt5051_init_mic_port(codec, 0x17, CXT5051_PORTB_EVENT);
@@ -2037,6 +2040,12 @@ static int patch_cxt5051(struct hda_codec *codec)
 	if (spec->beep_amp)
 		snd_hda_attach_beep_device(codec, spec->beep_amp);
 
+	conexant_init_jacks(codec);
+	if (spec->auto_mic & AUTO_MIC_PORTB)
+		cxt5051_init_mic_jack(codec, 0x17);
+	if (spec->auto_mic & AUTO_MIC_PORTC)
+		cxt5051_init_mic_jack(codec, 0x18);
+
 	return 0;
 }
 
-- 
1.7.9.4

