From 4a8252cb16f69ca39f21e3bf65064d70046adf38 Mon Sep 17 00:00:00 2001
From: Max Filippov <jcmvbkbc@gmail.com>
Date: Thu, 1 Mar 2012 00:40:08 +0400
Subject: [PATCH 047/147] p54spi: Release GPIO lines and IRQ on error in
 p54spi_probe

commit 62ebeed8d00aef75eac4fd6c161cae75a41965ca upstream.

This makes it possible to reload driver if insmod has failed due to
missing firmware.

Signed-off-by: Max Filippov <jcmvbkbc@gmail.com>
Acked-by: Christian Lamparter <chunkeey@googlemail.com>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/wireless/p54/p54spi.c |   14 ++++++++++----
 1 file changed, 10 insertions(+), 4 deletions(-)

diff --git a/drivers/net/wireless/p54/p54spi.c b/drivers/net/wireless/p54/p54spi.c
index 78d0d69..428401b 100644
--- a/drivers/net/wireless/p54/p54spi.c
+++ b/drivers/net/wireless/p54/p54spi.c
@@ -622,19 +622,19 @@ static int __devinit p54spi_probe(struct spi_device *spi)
 	ret = spi_setup(spi);
 	if (ret < 0) {
 		dev_err(&priv->spi->dev, "spi_setup failed");
-		goto err_free_common;
+		goto err_free;
 	}
 
 	ret = gpio_request(p54spi_gpio_power, "p54spi power");
 	if (ret < 0) {
 		dev_err(&priv->spi->dev, "power GPIO request failed: %d", ret);
-		goto err_free_common;
+		goto err_free;
 	}
 
 	ret = gpio_request(p54spi_gpio_irq, "p54spi irq");
 	if (ret < 0) {
 		dev_err(&priv->spi->dev, "irq GPIO request failed: %d", ret);
-		goto err_free_common;
+		goto err_free_gpio_power;
 	}
 
 	gpio_direction_output(p54spi_gpio_power, 0);
@@ -645,7 +645,7 @@ static int __devinit p54spi_probe(struct spi_device *spi)
 			  priv->spi);
 	if (ret < 0) {
 		dev_err(&priv->spi->dev, "request_irq() failed");
-		goto err_free_common;
+		goto err_free_gpio_irq;
 	}
 
 	irq_set_irq_type(gpio_to_irq(p54spi_gpio_irq), IRQ_TYPE_EDGE_RISING);
@@ -677,6 +677,12 @@ static int __devinit p54spi_probe(struct spi_device *spi)
 	return 0;
 
 err_free_common:
+	free_irq(gpio_to_irq(p54spi_gpio_irq), spi);
+err_free_gpio_irq:
+	gpio_free(p54spi_gpio_irq);
+err_free_gpio_power:
+	gpio_free(p54spi_gpio_power);
+err_free:
 	p54_free_common(priv->hw);
 	return ret;
 }
-- 
1.7.9.4

