From d32f43943a473899c4ac53710148f066ebc0d227 Mon Sep 17 00:00:00 2001
From: Yegor Yefremov <yegor_sub1@visionsystems.de>
Date: Mon, 23 Jan 2012 08:32:23 +0100
Subject: [PATCH 14/87] ARM: OMAP2+: GPMC: fix device size setup

commit 8ef5d844cc3a644ea6f7665932a4307e9fad01fa upstream.

following statement can only change device size from 8-bit(0) to 16-bit(1),
but not vice versa:

regval |= GPMC_CONFIG1_DEVICESIZE(wval);

so as this field has 1 reserved bit, that could be used in future,
just clear both bits and then OR with the desired value

Signed-off-by: Yegor Yefremov <yegorslists@googlemail.com>
Signed-off-by: Tony Lindgren <tony@atomide.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 arch/arm/mach-omap2/gpmc.c |    6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/arch/arm/mach-omap2/gpmc.c b/arch/arm/mach-omap2/gpmc.c
index a78f79d..9876c63 100644
--- a/arch/arm/mach-omap2/gpmc.c
+++ b/arch/arm/mach-omap2/gpmc.c
@@ -533,7 +533,13 @@ int gpmc_cs_configure(int cs, int cmd, int wval)
 
 	case GPMC_CONFIG_DEV_SIZE:
 		regval  = gpmc_cs_read_reg(cs, GPMC_CS_CONFIG1);
+
+		/* clear 2 target bits */
+		regval &= ~GPMC_CONFIG1_DEVICESIZE(3);
+
+		/* set the proper value */
 		regval |= GPMC_CONFIG1_DEVICESIZE(wval);
+
 		gpmc_cs_write_reg(cs, GPMC_CS_CONFIG1, regval);
 		break;
 
-- 
1.7.9.4

