From 97f236081bafdb80cac73ef005a6df79d4b2c803 Mon Sep 17 00:00:00 2001
From: Masanari Iida <standby24x7@gmail.com>
Date: Wed, 28 Mar 2012 14:42:56 -0700
Subject: [PATCH 123/147] backlight: fix typo in tosa_lcd.c

commit 8da00edc1069f01c34510fa405dc15d96c090a3f upstream.

Fix typo in drivers/video/backlight/tosa_lcd.c
"tosa_lcd_reume" should be "tosa_lcd_resume".

Signed-off-by: Masanari Iida <standby24x7@gmail.com>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/video/backlight/tosa_lcd.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/video/backlight/tosa_lcd.c b/drivers/video/backlight/tosa_lcd.c
index 772f601..6f54f74 100644
--- a/drivers/video/backlight/tosa_lcd.c
+++ b/drivers/video/backlight/tosa_lcd.c
@@ -271,7 +271,7 @@ static int tosa_lcd_resume(struct spi_device *spi)
 }
 #else
 #define tosa_lcd_suspend	NULL
-#define tosa_lcd_reume NULL
+#define tosa_lcd_resume NULL
 #endif
 
 static struct spi_driver tosa_lcd_driver = {
-- 
1.7.9.4

