From 22560ed5c9c2a4e693adf5981e47f3b5f363676d Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Tue, 17 Apr 2012 11:25:00 +0200
Subject: [PATCH 27/29] beaglebone: decrease PWM frequency to old value, LCD7
 doesn't like it

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index 74a7e91..b0ee67e 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -136,7 +136,7 @@ static const struct display_panel disp_panel = {
 /* LCD backlight platform Data */
 #define AM335X_BACKLIGHT_MAX_BRIGHTNESS        100
 #define AM335X_BACKLIGHT_DEFAULT_BRIGHTNESS    50
-#define AM335X_PWM_PERIOD_NANO_SECONDS        (5000 * 10)
+#define AM335X_PWM_PERIOD_NANO_SECONDS        (1000000 * 5)
 
 #define PWM_DEVICE_ID   "ecap.0"
 
-- 
1.7.7.6

