From a6ee86920e1888c173cabbc4e6dabfd12e68270b Mon Sep 17 00:00:00 2001
From: Nicolas Ferre <nicolas.ferre@atmel.com>
Date: Fri, 27 Jan 2012 11:14:44 +0100
Subject: [PATCH 03/72] ARM: at91: USB AT91 gadget registration for module

commit e8c9dc93e27d891636defbc269f182a83e6abba8 upstream.

Registration of at91_udc as a module will enable SoC
related code.

Fix following an idea from Karel Znamenacek.

Signed-off-by: Nicolas Ferre <nicolas.ferre@atmel.com>
Acked-by: Karel Znamenacek <karel@ryston.cz>
Acked-by: Jean-Christophe PLAGNIOL-VILLARD <plagnioj@jcrosoft.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 arch/arm/mach-at91/at91rm9200_devices.c  |    2 +-
 arch/arm/mach-at91/at91sam9260_devices.c |    2 +-
 arch/arm/mach-at91/at91sam9261_devices.c |    2 +-
 arch/arm/mach-at91/at91sam9263_devices.c |    2 +-
 4 files changed, 4 insertions(+), 4 deletions(-)

diff --git a/arch/arm/mach-at91/at91rm9200_devices.c b/arch/arm/mach-at91/at91rm9200_devices.c
index ad93068..143eebb 100644
--- a/arch/arm/mach-at91/at91rm9200_devices.c
+++ b/arch/arm/mach-at91/at91rm9200_devices.c
@@ -83,7 +83,7 @@ void __init at91_add_device_usbh(struct at91_usbh_data *data) {}
  *  USB Device (Gadget)
  * -------------------------------------------------------------------- */
 
-#ifdef CONFIG_USB_AT91
+#if defined(CONFIG_USB_AT91) || defined(CONFIG_USB_AT91_MODULE)
 static struct at91_udc_data udc_data;
 
 static struct resource udc_resources[] = {
diff --git a/arch/arm/mach-at91/at91sam9260_devices.c b/arch/arm/mach-at91/at91sam9260_devices.c
index 629fa97..2590988 100644
--- a/arch/arm/mach-at91/at91sam9260_devices.c
+++ b/arch/arm/mach-at91/at91sam9260_devices.c
@@ -84,7 +84,7 @@ void __init at91_add_device_usbh(struct at91_usbh_data *data) {}
  *  USB Device (Gadget)
  * -------------------------------------------------------------------- */
 
-#ifdef CONFIG_USB_AT91
+#if defined(CONFIG_USB_AT91) || defined(CONFIG_USB_AT91_MODULE)
 static struct at91_udc_data udc_data;
 
 static struct resource udc_resources[] = {
diff --git a/arch/arm/mach-at91/at91sam9261_devices.c b/arch/arm/mach-at91/at91sam9261_devices.c
index a178b58..daf3e66 100644
--- a/arch/arm/mach-at91/at91sam9261_devices.c
+++ b/arch/arm/mach-at91/at91sam9261_devices.c
@@ -87,7 +87,7 @@ void __init at91_add_device_usbh(struct at91_usbh_data *data) {}
  *  USB Device (Gadget)
  * -------------------------------------------------------------------- */
 
-#ifdef CONFIG_USB_AT91
+#if defined(CONFIG_USB_AT91) || defined(CONFIG_USB_AT91_MODULE)
 static struct at91_udc_data udc_data;
 
 static struct resource udc_resources[] = {
diff --git a/arch/arm/mach-at91/at91sam9263_devices.c b/arch/arm/mach-at91/at91sam9263_devices.c
index d5fbac9..32a7e43 100644
--- a/arch/arm/mach-at91/at91sam9263_devices.c
+++ b/arch/arm/mach-at91/at91sam9263_devices.c
@@ -92,7 +92,7 @@ void __init at91_add_device_usbh(struct at91_usbh_data *data) {}
  *  USB Device (Gadget)
  * -------------------------------------------------------------------- */
 
-#ifdef CONFIG_USB_AT91
+#if defined(CONFIG_USB_AT91) || defined(CONFIG_USB_AT91_MODULE)
 static struct at91_udc_data udc_data;
 
 static struct resource udc_resources[] = {
-- 
1.7.9.4

