From 407e1b9350ad2124952f769ade034023a9155c71 Mon Sep 17 00:00:00 2001
From: Roland Dreier <roland@purestorage.com>
Date: Thu, 23 Feb 2012 17:22:12 -0800
Subject: [PATCH 077/147] target: Fix 16-bit target ports for SET TARGET PORT
 GROUPS emulation

commit 33395fb8a13731c7ef7b175dbf5a4d8a6738fe6c upstream.

The old code did (MSB << 8) & 0xff, which always evaluates to 0.  Just use
get_unaligned_be16() so we don't have to worry about whether our open-coded
version is correct or not.

Signed-off-by: Roland Dreier <roland@purestorage.com>
Signed-off-by: Nicholas Bellinger <nab@linux-iscsi.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/target/target_core_alua.c |    7 +++----
 1 file changed, 3 insertions(+), 4 deletions(-)

diff --git a/drivers/target/target_core_alua.c b/drivers/target/target_core_alua.c
index 1d24512..5b05744 100644
--- a/drivers/target/target_core_alua.c
+++ b/drivers/target/target_core_alua.c
@@ -30,6 +30,7 @@
 #include <linux/export.h>
 #include <scsi/scsi.h>
 #include <scsi/scsi_cmnd.h>
+#include <asm/unaligned.h>
 
 #include <target/target_core_base.h>
 #include <target/target_core_device.h>
@@ -268,8 +269,7 @@ int target_emulate_set_target_port_groups(struct se_task *task)
 		 * changed.
 		 */
 		if (primary) {
-			tg_pt_id = ((ptr[2] << 8) & 0xff);
-			tg_pt_id |= (ptr[3] & 0xff);
+			tg_pt_id = get_unaligned_be16(ptr + 2);
 			/*
 			 * Locate the matching target port group ID from
 			 * the global tg_pt_gp list
@@ -313,8 +313,7 @@ int target_emulate_set_target_port_groups(struct se_task *task)
 			 * the Target Port in question for the the incoming
 			 * SET_TARGET_PORT_GROUPS op.
 			 */
-			rtpi = ((ptr[2] << 8) & 0xff);
-			rtpi |= (ptr[3] & 0xff);
+			rtpi = get_unaligned_be16(ptr + 2);
 			/*
 			 * Locate the matching relative target port identifer
 			 * for the struct se_device storage object.
-- 
1.7.9.4

