From 5f3ac99ec102297e3fa6be18ebc03d9ecde65d26 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Malte=20Schr=C3=B6der?= <maltesch@gmx.de>
Date: Thu, 5 Jan 2012 20:34:40 +0100
Subject: [PATCH 40/49] USB: Add USB-ID for Multiplex RC serial adapter to
 cp210x.c
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit 08e87d0d773dc9ca5faf4c3306e238ed0ea129b0 upstream.

Hi, below patch adds the USB-ID of the serial adapters sold by
Multiplex RC (www.multiplex-rc.de).

Signed-off-by: Malte Schröder <maltesch@gmx.de>
Cc: stable <stable@vger.kernel.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/usb/serial/cp210x.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/usb/serial/cp210x.c b/drivers/usb/serial/cp210x.c
index fd67cc5..a1a324b 100644
--- a/drivers/usb/serial/cp210x.c
+++ b/drivers/usb/serial/cp210x.c
@@ -92,6 +92,7 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(0x10C4, 0x818B) }, /* AVIT Research USB to TTL */
 	{ USB_DEVICE(0x10C4, 0x819F) }, /* MJS USB Toslink Switcher */
 	{ USB_DEVICE(0x10C4, 0x81A6) }, /* ThinkOptics WavIt */
+	{ USB_DEVICE(0x10C4, 0x81A9) }, /* Multiplex RC Interface */
 	{ USB_DEVICE(0x10C4, 0x81AC) }, /* MSD Dash Hawk */
 	{ USB_DEVICE(0x10C4, 0x81AD) }, /* INSYS USB Modem */
 	{ USB_DEVICE(0x10C4, 0x81C8) }, /* Lipowsky Industrie Elektronik GmbH, Baby-JTAG */
-- 
1.7.9.4

