From 2e80dec6dad3b037b7b6499048c139436c6f0710 Mon Sep 17 00:00:00 2001
From: Larry Finger <Larry.Finger@lwfinger.net>
Date: Mon, 26 Mar 2012 09:59:48 -0500
Subject: [PATCH 24/60] rtlwifi: rtl8192ce: rtl8192cu: rtl8192de: Fix low-gain
 setting when scanning

commit 643c61e119459e9d750087b7b34be94491efebf9 upstream.

In https://bugzilla.redhat.com/show_bug.cgi?id=770207, slowdowns of driver
rtl8192ce are reported. One fix (commit a9b89e2) has already been applied,
and it helped, but the maximum RX speed would still drop to 1 Mbps. As in
the previous fix, the initial gain was determined to be the problem; however,
the problem arises from a setting of the gain when scans are started.

Driver rtl8192de also has the same code structure - this one is fixed as well.

Reported-and-Tested-by: Ivan Pesin <ivan.pesin@gmail.com>
Signed-off-by: Larry Finger <Larry.Finger@lwfinger.net>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/wireless/rtlwifi/rtl8192c/phy_common.c |    2 +-
 drivers/net/wireless/rtlwifi/rtl8192de/phy.c       |    2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/net/wireless/rtlwifi/rtl8192c/phy_common.c b/drivers/net/wireless/rtlwifi/rtl8192c/phy_common.c
index 1f07558..f20678a 100644
--- a/drivers/net/wireless/rtlwifi/rtl8192c/phy_common.c
+++ b/drivers/net/wireless/rtlwifi/rtl8192c/phy_common.c
@@ -1968,7 +1968,7 @@ void rtl92c_phy_set_io(struct ieee80211_hw *hw)
 		break;
 	case IO_CMD_PAUSE_DM_BY_SCAN:
 		rtlphy->initgain_backup.xaagccore1 = dm_digtable.cur_igvalue;
-		dm_digtable.cur_igvalue = 0x17;
+		dm_digtable.cur_igvalue = 0x37;
 		rtl92c_dm_write_dig(hw);
 		break;
 	default:
diff --git a/drivers/net/wireless/rtlwifi/rtl8192de/phy.c b/drivers/net/wireless/rtlwifi/rtl8192de/phy.c
index 0883349..2cf4c5f 100644
--- a/drivers/net/wireless/rtlwifi/rtl8192de/phy.c
+++ b/drivers/net/wireless/rtlwifi/rtl8192de/phy.c
@@ -3192,7 +3192,7 @@ static void rtl92d_phy_set_io(struct ieee80211_hw *hw)
 		break;
 	case IO_CMD_PAUSE_DM_BY_SCAN:
 		rtlphy->initgain_backup.xaagccore1 = de_digtable.cur_igvalue;
-		de_digtable.cur_igvalue = 0x17;
+		de_digtable.cur_igvalue = 0x37;
 		rtl92d_dm_write_dig(hw);
 		break;
 	default:
-- 
1.7.9.5

