From bdab95dd61b9879afe660d0f5d97bf5b6ab0533e Mon Sep 17 00:00:00 2001
From: Gertjan van Wingerde <gwingerde@gmail.com>
Date: Sat, 11 Feb 2012 21:58:09 +0100
Subject: [PATCH 035/147] rt2x00: Add support for D-Link DWA-127 to rt2800usb.

commit d42a179b941a9e4cc6cf41d0f3cbadd75fc48a89 upstream.

This is an RT3070 based device.

Reported-by: Mikhail Kryshen <mikhail@kryshen.net>
Signed-off-by: Gertjan van Wingerde <gwingerde@gmail.com>
Acked-by: Ivo van Doorn <IvDoorn@gmail.com>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/wireless/rt2x00/rt2800usb.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/net/wireless/rt2x00/rt2800usb.c b/drivers/net/wireless/rt2x00/rt2800usb.c
index 3265b34..cb71e88 100644
--- a/drivers/net/wireless/rt2x00/rt2800usb.c
+++ b/drivers/net/wireless/rt2x00/rt2800usb.c
@@ -935,6 +935,7 @@ static struct usb_device_id rt2800usb_device_table[] = {
 	{ USB_DEVICE(0x07d1, 0x3c0f) },
 	{ USB_DEVICE(0x07d1, 0x3c11) },
 	{ USB_DEVICE(0x07d1, 0x3c16) },
+	{ USB_DEVICE(0x2001, 0x3c1b) },
 	/* Draytek */
 	{ USB_DEVICE(0x07fa, 0x7712) },
 	/* DVICO */
-- 
1.7.9.4

