From 6e85de6b5c1d71d372c23bf1f5c2388b9560f42f Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Wed, 25 May 2011 16:38:47 -0700
Subject: [PATCH 06/11] cpufreq: OMAP: deny initialization if no mpudev

if we do not have mpu_dev we normally fail in cpu_init. It is better
to fail driver registration if the devices are not available.

Signed-off-by: Nishanth Menon <nm@ti.com>
Signed-off-by: Kevin Hilman <khilman@ti.com>
---
 drivers/cpufreq/omap-cpufreq.c |   15 ++++++++-------
 1 files changed, 8 insertions(+), 7 deletions(-)

diff --git a/drivers/cpufreq/omap-cpufreq.c b/drivers/cpufreq/omap-cpufreq.c
index 3651825..dda32fd 100644
--- a/drivers/cpufreq/omap-cpufreq.c
+++ b/drivers/cpufreq/omap-cpufreq.c
@@ -50,6 +50,7 @@ static struct lpj_info global_lpj_ref;
 static struct cpufreq_frequency_table *freq_table;
 static struct clk *mpu_clk;
 static char *mpu_clk_name;
+static struct device *mpu_dev;
 
 static int omap_verify_speed(struct cpufreq_policy *policy)
 {
@@ -152,7 +153,6 @@ static int omap_target(struct cpufreq_policy *policy,
 static int __cpuinit omap_cpu_init(struct cpufreq_policy *policy)
 {
 	int result = 0;
-	struct device *mpu_dev;
 
 	mpu_clk = clk_get(NULL, mpu_clk_name);
 	if (IS_ERR(mpu_clk))
@@ -162,12 +162,6 @@ static int __cpuinit omap_cpu_init(struct cpufreq_policy *policy)
 		return -EINVAL;
 
 	policy->cur = policy->min = policy->max = omap_getspeed(policy->cpu);
-	mpu_dev = omap2_get_mpuss_device();
-
-	if (!mpu_dev) {
-		pr_warning("%s: unable to get the mpu device\n", __func__);
-		return -EINVAL;
-	}
 	opp_init_cpufreq_table(mpu_dev, &freq_table);
 
 	if (freq_table) {
@@ -239,6 +233,13 @@ static int __init omap_cpufreq_init(void)
 		pr_err("%s: unsupported Silicon?\n", __func__);
 		return -EINVAL;
 	}
+
+	mpu_dev = omap2_get_mpuss_device();
+	if (!mpu_dev) {
+		pr_warning("%s: unable to get the mpu device\n", __func__);
+		return -EINVAL;
+	}
+
 	return cpufreq_register_driver(&omap_driver);
 }
 
-- 
1.7.7.4

