From dd53a7c1ab8addfd2a943ea44b5ccc5700648323 Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Wed, 24 Feb 2010 10:37:22 -0800
Subject: [PATCH 26/28] ARM: OMAP: automatically set musb mode in platform data based on CONFIG options

---
 arch/arm/mach-omap2/board-omap3beagle.c |    6 ++++++
 arch/arm/mach-omap2/board-overo.c       |    6 ++++++
 2 files changed, 12 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 9259780..ad0c1d8 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -785,7 +785,13 @@ static struct omap_board_mux board_mux[] __initdata = {
 
 static struct omap_musb_board_data musb_board_data = {
 	.interface_type		= MUSB_INTERFACE_ULPI,
+#if defined(CONFIG_USB_MUSB_OTG)
 	.mode			= MUSB_OTG,
+#elif defined(CONFIG_USB_GADGET_MUSB_HDRC)
+	.mode			= MUSB_PERIPHERAL,
+#else
+	.mode			= MUSB_HOST,
+#endif
 	.power			= 100,
 };
 
diff --git a/arch/arm/mach-omap2/board-overo.c b/arch/arm/mach-omap2/board-overo.c
index 17f066a..b28a9d5 100644
--- a/arch/arm/mach-omap2/board-overo.c
+++ b/arch/arm/mach-omap2/board-overo.c
@@ -447,7 +447,13 @@ static struct omap_board_mux board_mux[] __initdata = {
 
 static struct omap_musb_board_data musb_board_data = {
 	.interface_type		= MUSB_INTERFACE_ULPI,
+#if defined(CONFIG_USB_MUSB_OTG)
 	.mode			= MUSB_OTG,
+#elif defined(CONFIG_USB_GADGET_MUSB_HDRC)
+	.mode			= MUSB_PERIPHERAL,
+#else
+	.mode			= MUSB_HOST,
+#endif
 	.power			= 100,
 };
 
-- 
1.6.6.1

