From d7ff9d198072099925dcc2bb81d17f1f08b0eba6 Mon Sep 17 00:00:00 2001
From: Harrison Metzger <harrisonmetz@gmail.com>
Date: Sun, 15 Jan 2012 08:43:24 -0600
Subject: [PATCH 56/90] USB: usbsevseg: fix max length

commit 1097ccebe630170080c41df0edcf88e0626e9c75 upstream.

This changes the max length for the usb seven segment delcom device to 8
from 6. Delcom has both 6 and 8 variants and having 8 works fine with
devices which are only 6.

Signed-off-by: Harrison Metzger <harrisonmetz@gmail.com>
Signed-off-by: Stuart Pook <stuart@acm.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/misc/usbsevseg.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/usb/misc/usbsevseg.c b/drivers/usb/misc/usbsevseg.c
index 417b8f2..59689fa 100644
--- a/drivers/usb/misc/usbsevseg.c
+++ b/drivers/usb/misc/usbsevseg.c
@@ -24,7 +24,7 @@
 
 #define VENDOR_ID	0x0fc5
 #define PRODUCT_ID	0x1227
-#define MAXLEN		6
+#define MAXLEN		8
 
 /* table of devices that work with this driver */
 static const struct usb_device_id id_table[] = {
-- 
1.7.9.4

