From e0781c37a52ef08a49e613ef22de8d28fa9cde4f Mon Sep 17 00:00:00 2001
From: Mark Brown <broonie@opensource.wolfsonmicro.com>
Date: Tue, 7 Feb 2012 17:24:19 +0000
Subject: [PATCH 60/87] ASoC: wm8994: Fix typo in VMID ramp setting

commit f647e1526fd6c7c8ab720781c40d11e11f930e93 upstream.

The VMID ramp rate is supposed to be 0x3, not 11b. Fix that.

Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/codecs/wm8994.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/codecs/wm8994.c b/sound/soc/codecs/wm8994.c
index a3d6bd8..6e502af 100644
--- a/sound/soc/codecs/wm8994.c
+++ b/sound/soc/codecs/wm8994.c
@@ -744,7 +744,7 @@ static void vmid_reference(struct snd_soc_codec *codec)
 				    WM8994_VMID_RAMP_MASK,
 				    WM8994_STARTUP_BIAS_ENA |
 				    WM8994_VMID_BUF_ENA |
-				    (0x11 << WM8994_VMID_RAMP_SHIFT));
+				    (0x3 << WM8994_VMID_RAMP_SHIFT));
 
 		/* Main bias enable, VMID=2x40k */
 		snd_soc_update_bits(codec, WM8994_POWER_MANAGEMENT_1,
-- 
1.7.9.4

