From 3168f6f46758c36d5b33ed5e77329bffed67033f Mon Sep 17 00:00:00 2001
From: Alex Deucher <alexander.deucher@amd.com>
Date: Tue, 10 Apr 2012 12:14:27 -0400
Subject: [PATCH 04/69] drm/radeon: only add the mm i2c bus if the hw_i2c
 module param is set

commit 46783150a6552f9513f08e62cfcc07125d6e502b upstream.

It seems it can corrupt the monitor EDID in certain cases on certain
boards when running sensors detect.  It's rarely used anyway outside
of AIW boards.

http://lists.lm-sensors.org/pipermail/lm-sensors/2012-April/035847.html
http://lists.freedesktop.org/archives/xorg/2011-January/052239.html

Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
Acked-by: Jean Delvare <khali@linux-fr.org>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/radeon/radeon_i2c.c |    4 ++++
 1 file changed, 4 insertions(+)

diff --git a/drivers/gpu/drm/radeon/radeon_i2c.c b/drivers/gpu/drm/radeon/radeon_i2c.c
index 7bb1b07..1441b00 100644
--- a/drivers/gpu/drm/radeon/radeon_i2c.c
+++ b/drivers/gpu/drm/radeon/radeon_i2c.c
@@ -890,6 +890,10 @@ struct radeon_i2c_chan *radeon_i2c_create(struct drm_device *dev,
 	struct radeon_i2c_chan *i2c;
 	int ret;
 
+	/* don't add the mm_i2c bus unless hw_i2c is enabled */
+	if (rec->mm_i2c && (radeon_hw_i2c == 0))
+		return NULL;
+
 	i2c = kzalloc(sizeof(struct radeon_i2c_chan), GFP_KERNEL);
 	if (i2c == NULL)
 		return NULL;
-- 
1.7.9.5

