From 99e22d6f848ffdc4e62916e92a41a4208b16a561 Mon Sep 17 00:00:00 2001
From: Johan Hovold <jhovold@gmail.com>
Date: Wed, 18 Jan 2012 01:46:00 +0100
Subject: [PATCH 41/90] USB: ftdi_sio: fix initial baud rate

commit 108e02b12921078a59dcacd048079ece48a4a983 upstream.

Fix regression introduced by commit b1ffb4c851f1 ("USB: Fix Corruption
issue in USB ftdi driver ftdi_sio.c") which caused the termios settings
to no longer be initialised at open. Consequently it was no longer
possible to set the port to the default speed of 9600 baud without first
changing to another baud rate and back again.

Reported-by: Roland Ramthun <mail@roland-ramthun.de>
Signed-off-by: Johan Hovold <jhovold@gmail.com>
Tested-by: Roland Ramthun <mail@roland-ramthun.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/serial/ftdi_sio.c |    7 +++++--
 1 file changed, 5 insertions(+), 2 deletions(-)

diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index 6a034b3..6a40b41 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -1823,6 +1823,7 @@ static int ftdi_sio_port_remove(struct usb_serial_port *port)
 
 static int ftdi_open(struct tty_struct *tty, struct usb_serial_port *port)
 {
+	struct ktermios dummy;
 	struct usb_device *dev = port->serial->dev;
 	struct ftdi_private *priv = usb_get_serial_port_data(port);
 	int result;
@@ -1841,8 +1842,10 @@ static int ftdi_open(struct tty_struct *tty, struct usb_serial_port *port)
 	   This is same behaviour as serial.c/rs_open() - Kuba */
 
 	/* ftdi_set_termios  will send usb control messages */
-	if (tty)
-		ftdi_set_termios(tty, port, tty->termios);
+	if (tty) {
+		memset(&dummy, 0, sizeof(dummy));
+		ftdi_set_termios(tty, port, &dummy);
+	}
 
 	/* Start reading from the device */
 	result = usb_serial_generic_open(tty, port);
-- 
1.7.9.4

