From f1a77f929e5e9c5399bf0e0a589280719f96654c Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Micha=C5=82=20Wr=C3=B3bel?= <michal.wrobel@flytronic.pl>
Date: Thu, 15 Mar 2012 17:24:04 +0100
Subject: [PATCH 011/147] USB: ftdi_sio: new PID: LUMEL PD12
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit 57e596f3af88ef52dea9640ed5e34ecd38893a02 upstream.

Signed-off-by: Micha?? Wr??bel <michal.wrobel@flytronic.pl>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/serial/ftdi_sio.c     |    1 +
 drivers/usb/serial/ftdi_sio_ids.h |    2 ++
 2 files changed, 3 insertions(+)

diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index b64fddc..3f3ccf6 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -849,6 +849,7 @@ static struct usb_device_id id_table_combined [] = {
 	{ USB_DEVICE(FTDI_VID, FTDI_RF_R106) },
 	{ USB_DEVICE(FTDI_VID, FTDI_DISTORTEC_JTAG_LOCK_PICK_PID),
 		.driver_info = (kernel_ulong_t)&ftdi_jtag_quirk },
+	{ USB_DEVICE(FTDI_VID, FTDI_LUMEL_PD12_PID) },
 	{ },					/* Optional parameter entry */
 	{ }					/* Terminating entry */
 };
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index ac1c42e..abf6bbc 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -30,6 +30,8 @@
 
 /*** third-party PIDs (using FTDI_VID) ***/
 
+#define FTDI_LUMEL_PD12_PID	0x6002
+
 /*
  * Marvell OpenRD Base, Client
  * http://www.open-rd.org
-- 
1.7.9.4

