From b9ec954fcea6867cd78e33f003ce6c11a8c1b217 Mon Sep 17 00:00:00 2001
From: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Date: Thu, 17 Nov 2011 16:14:23 +0900
Subject: [PATCH 59/69] pch_dma: Support new device LAPIS Semiconductor ML7831
 IOH

commit ca7fe2db892dcf91b2c72ee352eda4ff867903a7 upstream.

ML7831 is companion chip for Intel Atom E6xx series.

Signed-off-by: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Signed-off-by: Vinod Koul <vinod.koul@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/dma/Kconfig   |   13 ++++++-------
 drivers/dma/pch_dma.c |    8 ++++++--
 2 files changed, 12 insertions(+), 9 deletions(-)

diff --git a/drivers/dma/Kconfig b/drivers/dma/Kconfig
index 5a99bb3..da85c0d 100644
--- a/drivers/dma/Kconfig
+++ b/drivers/dma/Kconfig
@@ -201,18 +201,17 @@ config PL330_DMA
 	  platform_data for a dma-pl330 device.
 
 config PCH_DMA
-	tristate "Intel EG20T PCH / OKI Semi IOH(ML7213/ML7223) DMA support"
+	tristate "Intel EG20T PCH / OKI Semi IOH(ML7213/ML7223/ML7831) DMA support"
 	depends on PCI && X86
 	select DMA_ENGINE
 	help
 	  Enable support for Intel EG20T PCH DMA engine.
-
 	  This driver also can be used for OKI SEMICONDUCTOR IOH(Input/
-	  Output Hub), ML7213 and ML7223.
-	  ML7213 IOH is for IVI(In-Vehicle Infotainment) use and ML7223 IOH is
-	  for MP(Media Phone) use.
-	  ML7213/ML7223 is companion chip for Intel Atom E6xx series.
-	  ML7213/ML7223 is completely compatible for Intel EG20T PCH.
+	  Output Hub), ML7213, ML7223 and ML7831.
+	  ML7213 IOH is for IVI(In-Vehicle Infotainment) use, ML7223 IOH is
+	  for MP(Media Phone) use and ML7831 IOH is for general purpose use.
+	  ML7213/ML7223/ML7831 is companion chip for Intel Atom E6xx series.
+	  ML7213/ML7223/ML7831 is completely compatible for Intel EG20T PCH.
 
 config IMX_SDMA
 	tristate "i.MX SDMA support"
diff --git a/drivers/dma/pch_dma.c b/drivers/dma/pch_dma.c
index a6d0e3d..629c430 100644
--- a/drivers/dma/pch_dma.c
+++ b/drivers/dma/pch_dma.c
@@ -1018,6 +1018,8 @@ static void __devexit pch_dma_remove(struct pci_dev *pdev)
 #define PCI_DEVICE_ID_ML7223_DMA2_4CH	0x800E
 #define PCI_DEVICE_ID_ML7223_DMA3_4CH	0x8017
 #define PCI_DEVICE_ID_ML7223_DMA4_4CH	0x803B
+#define PCI_DEVICE_ID_ML7831_DMA1_8CH	0x8810
+#define PCI_DEVICE_ID_ML7831_DMA2_4CH	0x8815
 
 DEFINE_PCI_DEVICE_TABLE(pch_dma_id_table) = {
 	{ PCI_VDEVICE(INTEL, PCI_DEVICE_ID_EG20T_PCH_DMA_8CH), 8 },
@@ -1030,6 +1032,8 @@ DEFINE_PCI_DEVICE_TABLE(pch_dma_id_table) = {
 	{ PCI_VDEVICE(ROHM, PCI_DEVICE_ID_ML7223_DMA2_4CH), 4}, /* Video SPI */
 	{ PCI_VDEVICE(ROHM, PCI_DEVICE_ID_ML7223_DMA3_4CH), 4}, /* Security */
 	{ PCI_VDEVICE(ROHM, PCI_DEVICE_ID_ML7223_DMA4_4CH), 4}, /* FPGA */
+	{ PCI_VDEVICE(ROHM, PCI_DEVICE_ID_ML7831_DMA1_8CH), 8}, /* UART */
+	{ PCI_VDEVICE(ROHM, PCI_DEVICE_ID_ML7831_DMA2_4CH), 4}, /* SPI */
 	{ 0, },
 };
 
@@ -1057,7 +1061,7 @@ static void __exit pch_dma_exit(void)
 module_init(pch_dma_init);
 module_exit(pch_dma_exit);
 
-MODULE_DESCRIPTION("Intel EG20T PCH / OKI SEMICONDUCTOR ML7213 IOH "
-		   "DMA controller driver");
+MODULE_DESCRIPTION("Intel EG20T PCH / OKI SEMICON ML7213/ML7223/ML7831 IOH"
+			"DMA controller driver");
 MODULE_AUTHOR("Yong Wang <yong.y.wang@intel.com>");
 MODULE_LICENSE("GPL v2");
-- 
1.7.9.5

