From 113eac61d50555abefdb20ce9cebc839a2bc1968 Mon Sep 17 00:00:00 2001
From: Mark Brown <broonie@opensource.wolfsonmicro.com>
Date: Wed, 1 Feb 2012 23:46:58 +0000
Subject: [PATCH 57/87] ASoC: wm_hubs: Correct line input to line output 2
 paths

commit 43b6cec27e1e50a1de3eff47e66e502f3fe7e66e upstream.

The second line output mixer has the controls for the line input bypasses
in the opposite order.

Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/codecs/wm_hubs.c |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/sound/soc/codecs/wm_hubs.c b/sound/soc/codecs/wm_hubs.c
index 6ef2283..3642e06 100644
--- a/sound/soc/codecs/wm_hubs.c
+++ b/sound/soc/codecs/wm_hubs.c
@@ -587,8 +587,8 @@ SOC_DAPM_SINGLE("Left Output Switch", WM8993_LINE_MIXER1, 0, 1, 0),
 };
 
 static const struct snd_kcontrol_new line2_mix[] = {
-SOC_DAPM_SINGLE("IN1R Switch", WM8993_LINE_MIXER2, 2, 1, 0),
-SOC_DAPM_SINGLE("IN1L Switch", WM8993_LINE_MIXER2, 1, 1, 0),
+SOC_DAPM_SINGLE("IN1L Switch", WM8993_LINE_MIXER2, 2, 1, 0),
+SOC_DAPM_SINGLE("IN1R Switch", WM8993_LINE_MIXER2, 1, 1, 0),
 SOC_DAPM_SINGLE("Output Switch", WM8993_LINE_MIXER2, 0, 1, 0),
 };
 
-- 
1.7.9.4

