From 9200ef1704e7415a883be5ff751f486da1df7212 Mon Sep 17 00:00:00 2001
From: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Date: Thu, 12 Jan 2012 11:27:08 +0900
Subject: [PATCH 53/69] usb: gadget: pch_udc: Fix usb/gadget/pch_udc: Fix
 ether gadget connect/disconnect issue

commit 1c575d2d2e3ff2a7cb3c2e2165064199cfd8ad32 upstream.

ISSUE:
After a USB cable is connect/disconnected, the system rarely freezes.

CAUSE:
Since the USB device controller cannot know to disconnect the USB cable, when
it is used without detecting VBUS by GPIO, the UDC driver does not notify to
USB Gadget.

Since USB Gadget cannot know to disconnect, a false setting occurred when the
USB cable is connected/disconnect repeatedly.

Signed-off-by: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/gadget/pch_udc.c |   70 +++++++++++++++++++++++++++++++++++++++---
 1 file changed, 66 insertions(+), 4 deletions(-)

diff --git a/drivers/usb/gadget/pch_udc.c b/drivers/usb/gadget/pch_udc.c
index 3ab799c..f232e65 100644
--- a/drivers/usb/gadget/pch_udc.c
+++ b/drivers/usb/gadget/pch_udc.c
@@ -311,6 +311,7 @@ struct pch_udc_ep {
  * @registered:		driver regsitered with system
  * @suspended:		driver in suspended state
  * @connected:		gadget driver associated
+ * @vbus_session:	required vbus_session state
  * @set_cfg_not_acked:	pending acknowledgement 4 setup
  * @waiting_zlp_ack:	pending acknowledgement 4 ZLP
  * @data_requests:	DMA pool for data requests
@@ -337,6 +338,7 @@ struct pch_udc_dev {
 			registered:1,
 			suspended:1,
 			connected:1,
+			vbus_session:1,
 			set_cfg_not_acked:1,
 			waiting_zlp_ack:1;
 	struct pci_pool		*data_requests;
@@ -554,6 +556,31 @@ static void pch_udc_clear_disconnect(struct pch_udc_dev *dev)
 }
 
 /**
+ * pch_udc_reconnect() - This API initializes usb device controller,
+ *						and clear the disconnect status.
+ * @dev:		Reference to pch_udc_regs structure
+ */
+static void pch_udc_init(struct pch_udc_dev *dev);
+static void pch_udc_reconnect(struct pch_udc_dev *dev)
+{
+	pch_udc_init(dev);
+
+	/* enable device interrupts */
+	/* pch_udc_enable_interrupts() */
+	pch_udc_bit_clr(dev, UDC_DEVIRQMSK_ADDR,
+			UDC_DEVINT_UR | UDC_DEVINT_US |
+			UDC_DEVINT_ENUM |
+			UDC_DEVINT_SI | UDC_DEVINT_SC);
+
+	/* Clear the disconnect */
+	pch_udc_bit_set(dev, UDC_DEVCTL_ADDR, UDC_DEVCTL_RES);
+	pch_udc_bit_clr(dev, UDC_DEVCTL_ADDR, UDC_DEVCTL_SD);
+	mdelay(1);
+	/* Resume USB signalling */
+	pch_udc_bit_clr(dev, UDC_DEVCTL_ADDR, UDC_DEVCTL_RES);
+}
+
+/**
  * pch_udc_vbus_session() - set or clearr the disconnect status.
  * @dev:	Reference to pch_udc_regs structure
  * @is_active:	Parameter specifying the action
@@ -563,10 +590,18 @@ static void pch_udc_clear_disconnect(struct pch_udc_dev *dev)
 static inline void pch_udc_vbus_session(struct pch_udc_dev *dev,
 					  int is_active)
 {
-	if (is_active)
-		pch_udc_clear_disconnect(dev);
-	else
+	if (is_active) {
+		pch_udc_reconnect(dev);
+		dev->vbus_session = 1;
+	} else {
+		if (dev->driver && dev->driver->disconnect) {
+			spin_unlock(&dev->lock);
+			dev->driver->disconnect(&dev->gadget);
+			spin_lock(&dev->lock);
+		}
 		pch_udc_set_disconnect(dev);
+		dev->vbus_session = 0;
+	}
 }
 
 /**
@@ -1126,7 +1161,17 @@ static int pch_udc_pcd_pullup(struct usb_gadget *gadget, int is_on)
 	if (!gadget)
 		return -EINVAL;
 	dev = container_of(gadget, struct pch_udc_dev, gadget);
-	pch_udc_vbus_session(dev, is_on);
+	if (is_on) {
+		pch_udc_reconnect(dev);
+	} else {
+		if (dev->driver && dev->driver->disconnect) {
+			spin_unlock(&dev->lock);
+			dev->driver->disconnect(&dev->gadget);
+			spin_lock(&dev->lock);
+		}
+		pch_udc_set_disconnect(dev);
+	}
+
 	return 0;
 }
 
@@ -2482,6 +2527,15 @@ static void pch_udc_dev_isr(struct pch_udc_dev *dev, u32 dev_intr)
 			dev->driver->suspend(&dev->gadget);
 			spin_lock(&dev->lock);
 		}
+
+		if (dev->vbus_session == 0) {
+			if (dev->driver && dev->driver->disconnect) {
+				spin_unlock(&dev->lock);
+				dev->driver->disconnect(&dev->gadget);
+				spin_lock(&dev->lock);
+			}
+			pch_udc_reconnect(dev);
+		}
 		dev_dbg(&dev->pdev->dev, "USB_SUSPEND\n");
 	}
 	/* Clear the SOF interrupt, if enabled */
@@ -2509,6 +2563,14 @@ static irqreturn_t pch_udc_isr(int irq, void *pdev)
 	dev_intr = pch_udc_read_device_interrupts(dev);
 	ep_intr = pch_udc_read_ep_interrupts(dev);
 
+	/* For a hot plug, this find that the controller is hung up. */
+	if (dev_intr == ep_intr)
+		if (dev_intr == pch_udc_readl(dev, UDC_DEVCFG_ADDR)) {
+			dev_dbg(&dev->pdev->dev, "UDC: Hung up\n");
+			/* The controller is reset */
+			pch_udc_writel(dev, UDC_SRST, UDC_SRST_ADDR);
+			return IRQ_HANDLED;
+		}
 	if (dev_intr)
 		/* Clear device interrupts */
 		pch_udc_write_device_interrupts(dev, dev_intr);
-- 
1.7.9.5

