From 7e5aab3ce9f6ddf8e33efb988160d61011857f64 Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Thu, 26 Jan 2012 15:56:16 +0100
Subject: [PATCH 29/90] ALSA: hda - Fix silent output on Haier W18 laptop

commit b3a81520bd37a28f77cb0f7002086fb14061824d upstream.

The very same problem is seen on Haier W18 laptop with ALC861 as seen
on ASUS A6Rp, which was fixed by the commit 3b25eb69.
Now we just need to add a new SSID entry pointing to the same fixup.

Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=42656

Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/pci/hda/patch_realtek.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/sound/pci/hda/patch_realtek.c b/sound/pci/hda/patch_realtek.c
index 9a63a19..5f03c40 100644
--- a/sound/pci/hda/patch_realtek.c
+++ b/sound/pci/hda/patch_realtek.c
@@ -5247,6 +5247,7 @@ static const struct alc_fixup alc861_fixups[] = {
 
 static const struct snd_pci_quirk alc861_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x1043, 0x1393, "ASUS A6Rp", PINFIX_ASUS_A6RP),
+	SND_PCI_QUIRK(0x1584, 0x2b01, "Haier W18", PINFIX_ASUS_A6RP),
 	SND_PCI_QUIRK(0x1734, 0x10c7, "FSC Amilo Pi1505", PINFIX_FSC_AMILO_PI1505),
 	{}
 };
-- 
1.7.9.4

