From be6768ee3f1d5ade04946ae2d9b9642e795b4dc3 Mon Sep 17 00:00:00 2001
From: Mark Brown <broonie@opensource.wolfsonmicro.com>
Date: Wed, 21 Mar 2012 13:22:40 +0000
Subject: [PATCH 07/60] ASoC: wm8994: Update WM8994 DCS calibration

commit e16605855d58803fe0608417150c7a618b4f8243 upstream.

Based on latest production information.

Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/codecs/wm8994.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/codecs/wm8994.c b/sound/soc/codecs/wm8994.c
index 6e502af..2f1f5f8 100644
--- a/sound/soc/codecs/wm8994.c
+++ b/sound/soc/codecs/wm8994.c
@@ -3190,7 +3190,7 @@ static int wm8994_codec_probe(struct snd_soc_codec *codec)
 		case 2:
 		case 3:
 			wm8994->hubs.dcs_codes_l = -9;
-			wm8994->hubs.dcs_codes_r = -5;
+			wm8994->hubs.dcs_codes_r = -7;
 			break;
 		default:
 			break;
-- 
1.7.9.5

