From fd9b7416ae26e584935f0a1fdf215fb318c54b07 Mon Sep 17 00:00:00 2001
From: Paolo Bonzini <pbonzini@redhat.com>
Date: Thu, 12 Jan 2012 16:01:27 +0100
Subject: [PATCH 090/130] block: add and use scsi_blk_cmd_ioctl

commit 577ebb374c78314ac4617242f509e2f5e7156649 upstream.

Introduce a wrapper around scsi_cmd_ioctl that takes a block device.

The function will then be enhanced to detect partition block devices
and, in that case, subject the ioctls to whitelisting.

Cc: linux-scsi@vger.kernel.org
Cc: Jens Axboe <axboe@kernel.dk>
Cc: James Bottomley <JBottomley@parallels.com>
Signed-off-by: Paolo Bonzini <pbonzini@redhat.com>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 block/scsi_ioctl.c             |    7 +++++++
 drivers/block/cciss.c          |    6 +++---
 drivers/block/ub.c             |    3 +--
 drivers/block/virtio_blk.c     |    4 ++--
 drivers/cdrom/cdrom.c          |    3 +--
 drivers/ide/ide-floppy_ioctl.c |    3 +--
 drivers/scsi/sd.c              |    2 +-
 include/linux/blkdev.h         |    2 ++
 8 files changed, 18 insertions(+), 12 deletions(-)

diff --git a/block/scsi_ioctl.c b/block/scsi_ioctl.c
index fbdf0d8..a2c11f3 100644
--- a/block/scsi_ioctl.c
+++ b/block/scsi_ioctl.c
@@ -690,6 +690,13 @@ int scsi_cmd_ioctl(struct request_queue *q, struct gendisk *bd_disk, fmode_t mod
 }
 EXPORT_SYMBOL(scsi_cmd_ioctl);
 
+int scsi_cmd_blk_ioctl(struct block_device *bd, fmode_t mode,
+		       unsigned int cmd, void __user *arg)
+{
+	return scsi_cmd_ioctl(bd->bd_disk->queue, bd->bd_disk, mode, cmd, arg);
+}
+EXPORT_SYMBOL(scsi_cmd_blk_ioctl);
+
 static int __init blk_scsi_ioctl_init(void)
 {
 	blk_set_cmd_filter_defaults(&blk_default_cmd_filter);
diff --git a/drivers/block/cciss.c b/drivers/block/cciss.c
index 587cce5..b0f553b 100644
--- a/drivers/block/cciss.c
+++ b/drivers/block/cciss.c
@@ -1735,7 +1735,7 @@ static int cciss_ioctl(struct block_device *bdev, fmode_t mode,
 	case CCISS_BIG_PASSTHRU:
 		return cciss_bigpassthru(h, argp);
 
-	/* scsi_cmd_ioctl handles these, below, though some are not */
+	/* scsi_cmd_blk_ioctl handles these, below, though some are not */
 	/* very meaningful for cciss.  SG_IO is the main one people want. */
 
 	case SG_GET_VERSION_NUM:
@@ -1746,9 +1746,9 @@ static int cciss_ioctl(struct block_device *bdev, fmode_t mode,
 	case SG_EMULATED_HOST:
 	case SG_IO:
 	case SCSI_IOCTL_SEND_COMMAND:
-		return scsi_cmd_ioctl(disk->queue, disk, mode, cmd, argp);
+		return scsi_cmd_blk_ioctl(bdev, mode, cmd, argp);
 
-	/* scsi_cmd_ioctl would normally handle these, below, but */
+	/* scsi_cmd_blk_ioctl would normally handle these, below, but */
 	/* they aren't a good fit for cciss, as CD-ROMs are */
 	/* not supported, and we don't have any bus/target/lun */
 	/* which we present to the kernel. */
diff --git a/drivers/block/ub.c b/drivers/block/ub.c
index 0e376d4..7333b9e 100644
--- a/drivers/block/ub.c
+++ b/drivers/block/ub.c
@@ -1744,12 +1744,11 @@ static int ub_bd_release(struct gendisk *disk, fmode_t mode)
 static int ub_bd_ioctl(struct block_device *bdev, fmode_t mode,
     unsigned int cmd, unsigned long arg)
 {
-	struct gendisk *disk = bdev->bd_disk;
 	void __user *usermem = (void __user *) arg;
 	int ret;
 
 	mutex_lock(&ub_mutex);
-	ret = scsi_cmd_ioctl(disk->queue, disk, mode, cmd, usermem);
+	ret = scsi_cmd_blk_ioctl(bdev, mode, cmd, usermem);
 	mutex_unlock(&ub_mutex);
 
 	return ret;
diff --git a/drivers/block/virtio_blk.c b/drivers/block/virtio_blk.c
index 4d0b70a..e46f2f7 100644
--- a/drivers/block/virtio_blk.c
+++ b/drivers/block/virtio_blk.c
@@ -243,8 +243,8 @@ static int virtblk_ioctl(struct block_device *bdev, fmode_t mode,
 	if (!virtio_has_feature(vblk->vdev, VIRTIO_BLK_F_SCSI))
 		return -ENOTTY;
 
-	return scsi_cmd_ioctl(disk->queue, disk, mode, cmd,
-			      (void __user *)data);
+	return scsi_cmd_blk_ioctl(bdev, mode, cmd,
+				  (void __user *)data);
 }
 
 /* We provide getgeo only to please some old bootloader/partitioning tools */
diff --git a/drivers/cdrom/cdrom.c b/drivers/cdrom/cdrom.c
index f997c27..cedb231 100644
--- a/drivers/cdrom/cdrom.c
+++ b/drivers/cdrom/cdrom.c
@@ -2747,12 +2747,11 @@ int cdrom_ioctl(struct cdrom_device_info *cdi, struct block_device *bdev,
 {
 	void __user *argp = (void __user *)arg;
 	int ret;
-	struct gendisk *disk = bdev->bd_disk;
 
 	/*
 	 * Try the generic SCSI command ioctl's first.
 	 */
-	ret = scsi_cmd_ioctl(disk->queue, disk, mode, cmd, argp);
+	ret = scsi_cmd_blk_ioctl(bdev, mode, cmd, argp);
 	if (ret != -ENOTTY)
 		return ret;
 
diff --git a/drivers/ide/ide-floppy_ioctl.c b/drivers/ide/ide-floppy_ioctl.c
index d267b7a..a22ca84 100644
--- a/drivers/ide/ide-floppy_ioctl.c
+++ b/drivers/ide/ide-floppy_ioctl.c
@@ -292,8 +292,7 @@ int ide_floppy_ioctl(ide_drive_t *drive, struct block_device *bdev,
 	 * and CDROM_SEND_PACKET (legacy) ioctls
 	 */
 	if (cmd != CDROM_SEND_PACKET && cmd != SCSI_IOCTL_SEND_COMMAND)
-		err = scsi_cmd_ioctl(bdev->bd_disk->queue, bdev->bd_disk,
-				mode, cmd, argp);
+		err = scsi_cmd_blk_ioctl(bdev, mode, cmd, argp);
 
 	if (err == -ENOTTY)
 		err = generic_ide_ioctl(drive, bdev, cmd, arg);
diff --git a/drivers/scsi/sd.c b/drivers/scsi/sd.c
index fa3a591..ffa1c79 100644
--- a/drivers/scsi/sd.c
+++ b/drivers/scsi/sd.c
@@ -1096,7 +1096,7 @@ static int sd_ioctl(struct block_device *bdev, fmode_t mode,
 			error = scsi_ioctl(sdp, cmd, p);
 			break;
 		default:
-			error = scsi_cmd_ioctl(disk->queue, disk, mode, cmd, p);
+			error = scsi_cmd_blk_ioctl(bdev, mode, cmd, p);
 			if (error != -ENOTTY)
 				break;
 			error = scsi_ioctl(sdp, cmd, p);
diff --git a/include/linux/blkdev.h b/include/linux/blkdev.h
index 94acd81..ca7b869 100644
--- a/include/linux/blkdev.h
+++ b/include/linux/blkdev.h
@@ -675,6 +675,8 @@ extern int blk_insert_cloned_request(struct request_queue *q,
 				     struct request *rq);
 extern void blk_delay_queue(struct request_queue *, unsigned long);
 extern void blk_recount_segments(struct request_queue *, struct bio *);
+extern int scsi_cmd_blk_ioctl(struct block_device *, fmode_t,
+			      unsigned int, void __user *);
 extern int scsi_cmd_ioctl(struct request_queue *, struct gendisk *, fmode_t,
 			  unsigned int, void __user *);
 extern int sg_scsi_ioctl(struct request_queue *, struct gendisk *, fmode_t,
-- 
1.7.9.4

