From 072d0e473d1a1d4adc67a7d39be9f71fea4fadad Mon Sep 17 00:00:00 2001
From: Toshiharu Okada <toshiharu-linux@dsn.okisemi.com>
Date: Mon, 26 Sep 2011 16:16:23 +0900
Subject: [PATCH 119/129] i2c-eg20t: modified the setting of transfer rate.

commit ff35e8b18984ad2a82cbd259fc07f0be4b34b1aa upstream.

This patch modified the setting value of
I2C Bus Transfer Rate Setting Counter regisrer.

Signed-off-by: Toshiharu Okada <toshiharu-linux@dsn.okisemi.com>
Signed-off-by: Ben Dooks <ben-linux@fluff.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/i2c/busses/i2c-eg20t.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/i2c/busses/i2c-eg20t.c b/drivers/i2c/busses/i2c-eg20t.c
index 18936ac..730215e 100644
--- a/drivers/i2c/busses/i2c-eg20t.c
+++ b/drivers/i2c/busses/i2c-eg20t.c
@@ -243,7 +243,7 @@ static void pch_i2c_init(struct i2c_algo_pch_data *adap)
 	if (pch_clk > PCH_MAX_CLK)
 		pch_clk = 62500;
 
-	pch_i2cbc = (pch_clk + (pch_i2c_speed * 4)) / pch_i2c_speed * 8;
+	pch_i2cbc = (pch_clk + (pch_i2c_speed * 4)) / (pch_i2c_speed * 8);
 	/* Set transfer speed in I2CBC */
 	iowrite32(pch_i2cbc, p + PCH_I2CBC);
 
-- 
1.7.9.5

