From 037ef3add42d61dcd86438dc4b9378f154caa426 Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Thu, 23 Sep 2010 18:22:48 -0700
Subject: [PATCH 03/10] omap: Beagle: no gpio_wp pin connection on xM

The omap3630 based BeagleBoard xM uses a MicroSD card slot with
no write protection.

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
Acked-by: Jarkko Nikula <jhnikula@gmail.com>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    4 +++-
 1 files changed, 3 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index beb877c..247a426 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -444,7 +444,9 @@ static struct gpio_led gpio_leds[];
 static int beagle_twl_gpio_setup(struct device *dev,
 		unsigned gpio, unsigned ngpio)
 {
-	if ((omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_C1_3) ||
+	if (omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_XM) {
+		mmc[0].gpio_wp = -EINVAL;
+	} else if ((omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_C1_3) ||
 		(omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_C4)) {
 		omap_mux_init_gpio(23, OMAP_PIN_INPUT);
 		mmc[0].gpio_wp = 23;
-- 
1.6.6.1

