From 0532e1f8a710f011e839ad1ad0d83c6f3a1d2d74 Mon Sep 17 00:00:00 2001
From: Dave Airlie <airlied@redhat.com>
Date: Fri, 13 Apr 2012 11:14:50 +0100
Subject: [PATCH 67/69] drm/radeon: disable MSI on RV515

commit 16a5e32b83fd946312b9b13590c75d20c95c5202 upstream.

My rv515 card is very flaky with msi enabled. Every so often it loses a rearm
and never comes back, manually banging the rearm brings it back.

Reviewed-by: Alex Deucher <alexander.deucher@amd.com>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/radeon/radeon_irq_kms.c |    6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/drivers/gpu/drm/radeon/radeon_irq_kms.c b/drivers/gpu/drm/radeon/radeon_irq_kms.c
index e7ddb49..baa019e 100644
--- a/drivers/gpu/drm/radeon/radeon_irq_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_irq_kms.c
@@ -143,6 +143,12 @@ static bool radeon_msi_ok(struct radeon_device *rdev)
 	    (rdev->pdev->subsystem_device == 0x01fd))
 		return true;
 
+	/* RV515 seems to have MSI issues where it loses
+	 * MSI rearms occasionally. This leads to lockups and freezes.
+	 * disable it by default.
+	 */
+	if (rdev->family == CHIP_RV515)
+		return false;
 	if (rdev->flags & RADEON_IS_IGP) {
 		/* APUs work fine with MSIs */
 		if (rdev->family >= CHIP_PALM)
-- 
1.7.9.5

