From 841c06ccc583055a42b0546efb5e6b448f26d5fd Mon Sep 17 00:00:00 2001
From: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Date: Thu, 12 Jan 2012 11:27:09 +0900
Subject: [PATCH 54/69] usb: gadget: pch_udc: Reduce redundant interrupt

commit 833310402c54ad9b676b465fc53ad276b13d36be upstream.

ISSUE:
USB Suspend interrupts occur frequently.

CAUSE:
When it is called pch_udc_reconnect() in USB Suspend, it repeats reset and
Suspend.

SOLUTION:
pch_udc_reconnect() does not enable all interrupts.  When an enumeration event
occurred the driver enables all interrupts.

Signed-off-by: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/gadget/pch_udc.c |    9 ++++++---
 1 file changed, 6 insertions(+), 3 deletions(-)

diff --git a/drivers/usb/gadget/pch_udc.c b/drivers/usb/gadget/pch_udc.c
index f232e65..870897ac 100644
--- a/drivers/usb/gadget/pch_udc.c
+++ b/drivers/usb/gadget/pch_udc.c
@@ -568,9 +568,7 @@ static void pch_udc_reconnect(struct pch_udc_dev *dev)
 	/* enable device interrupts */
 	/* pch_udc_enable_interrupts() */
 	pch_udc_bit_clr(dev, UDC_DEVIRQMSK_ADDR,
-			UDC_DEVINT_UR | UDC_DEVINT_US |
-			UDC_DEVINT_ENUM |
-			UDC_DEVINT_SI | UDC_DEVINT_SC);
+			UDC_DEVINT_UR | UDC_DEVINT_ENUM);
 
 	/* Clear the disconnect */
 	pch_udc_bit_set(dev, UDC_DEVCTL_ADDR, UDC_DEVCTL_RES);
@@ -2419,6 +2417,11 @@ static void pch_udc_svc_enum_interrupt(struct pch_udc_dev *dev)
 	pch_udc_set_dma(dev, DMA_DIR_TX);
 	pch_udc_set_dma(dev, DMA_DIR_RX);
 	pch_udc_ep_set_rrdy(&(dev->ep[UDC_EP0OUT_IDX]));
+
+	/* enable device interrupts */
+	pch_udc_enable_interrupts(dev, UDC_DEVINT_UR | UDC_DEVINT_US |
+					UDC_DEVINT_ES | UDC_DEVINT_ENUM |
+					UDC_DEVINT_SI | UDC_DEVINT_SC);
 }
 
 /**
-- 
1.7.9.5

