From 55315e3442ea08e4bd0d676921f968dc1fccf588 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 1 Feb 2012 14:10:38 +0100
Subject: [PATCH 17/26] beaglebone: set default brightness to 50% for pwm
 backlights

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index 23b59c2..9294af5 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -133,7 +133,7 @@ static const struct display_panel disp_panel = {
 
 /* LCD backlight platform Data */
 #define AM335X_BACKLIGHT_MAX_BRIGHTNESS        100
-#define AM335X_BACKLIGHT_DEFAULT_BRIGHTNESS    100
+#define AM335X_BACKLIGHT_DEFAULT_BRIGHTNESS    50
 #define AM335X_PWM_PERIOD_NANO_SECONDS        (5000 * 10)
 
 #define PWM_DEVICE_ID   "ecap.0"
-- 
1.7.9.5

