From 7d3eb8bf92abead3bd005400d600f32ea4bf9d63 Mon Sep 17 00:00:00 2001
From: Rabin Vincent <rabin.vincent@stericsson.com>
Date: Tue, 22 Nov 2011 11:03:14 +0100
Subject: [PATCH 046/147] rtc: Disable the alarm in the hardware (v2)

commit 41c7f7424259ff11009449f87c95656f69f9b186 upstream.

Currently, the RTC code does not disable the alarm in the hardware.

This means that after a sequence such as the one below (the files are in the
RTC sysfs), the box will boot up after 2 minutes even though we've
asked for the alarm to be turned off.

	# echo $((`cat since_epoch`)+120) > wakealarm
	# echo 0 > wakealarm
	# poweroff

Fix this by disabling the alarm when there are no timers to run.

The original version of this patch was reverted. This version
disables the irq directly instead of setting a disabled timer
in the future.

Cc: John Stultz <john.stultz@linaro.org>
Signed-off-by: Rabin Vincent <rabin.vincent@stericsson.com>
[Merged in the second revision from Rabin]
Signed-off-by: John Stultz <john.stultz@linaro.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/rtc/interface.c |   15 +++++++++++++--
 1 file changed, 13 insertions(+), 2 deletions(-)

diff --git a/drivers/rtc/interface.c b/drivers/rtc/interface.c
index 8a1c031..c1edbf8 100644
--- a/drivers/rtc/interface.c
+++ b/drivers/rtc/interface.c
@@ -763,6 +763,14 @@ static int rtc_timer_enqueue(struct rtc_device *rtc, struct rtc_timer *timer)
 	return 0;
 }
 
+static void rtc_alarm_disable(struct rtc_device *rtc)
+{
+	if (!rtc->ops || !rtc->ops->alarm_irq_enable)
+		return;
+
+	rtc->ops->alarm_irq_enable(rtc->dev.parent, false);
+}
+
 /**
  * rtc_timer_remove - Removes a rtc_timer from the rtc_device timerqueue
  * @rtc rtc device
@@ -784,8 +792,10 @@ static void rtc_timer_remove(struct rtc_device *rtc, struct rtc_timer *timer)
 		struct rtc_wkalrm alarm;
 		int err;
 		next = timerqueue_getnext(&rtc->timerqueue);
-		if (!next)
+		if (!next) {
+			rtc_alarm_disable(rtc);
 			return;
+		}
 		alarm.time = rtc_ktime_to_tm(next->expires);
 		alarm.enabled = 1;
 		err = __rtc_set_alarm(rtc, &alarm);
@@ -847,7 +857,8 @@ again:
 		err = __rtc_set_alarm(rtc, &alarm);
 		if (err == -ETIME)
 			goto again;
-	}
+	} else
+		rtc_alarm_disable(rtc);
 
 	mutex_unlock(&rtc->ops_lock);
 }
-- 
1.7.9.4

