From 6408483ea69660e6ad8a2a8852edb9cd539cd51d Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Tue, 13 Mar 2012 13:27:23 +0100
Subject: [PATCH 42/69] serial: PL011: clear pending interrupts

commit 9b96fbacda34079dea0638ee1e92c56286f6114a upstream.

Chanho Min reported that when the boot loader transfers
control to the kernel, there may be pending interrupts
causing the UART to lock up in an eternal loop trying to
pick tokens from the FIFO (since the RX interrupt flag
indicates there are tokens) while in practice there are
no tokens - in fact there is only a pending IRQ flag.

This patch address the issue with a combination of two
patches suggested by Russell King that clears and mask
all interrupts at probe() and clears any pending error
and RX interrupts at port startup time.

We suspect the spurious interrupts are a side-effect of
switching the UART from FIFO to non-FIFO mode.

Cc: Shreshtha Kumar Sahu <shreshthakumar.sahu@stericsson.com>
Reported-by: Chanho Min <chanho0207@gmail.com>
Suggested-by: Russell King <linux@arm.linux.org.uk>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Reviewed-by: Jong-Sung Kim <neidhard.kim@lge.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/tty/serial/amba-pl011.c |   15 +++++++++++----
 1 file changed, 11 insertions(+), 4 deletions(-)

diff --git a/drivers/tty/serial/amba-pl011.c b/drivers/tty/serial/amba-pl011.c
index 8e00926..dddc3f2 100644
--- a/drivers/tty/serial/amba-pl011.c
+++ b/drivers/tty/serial/amba-pl011.c
@@ -1380,6 +1380,10 @@ static int pl011_startup(struct uart_port *port)
 
 	uap->port.uartclk = clk_get_rate(uap->clk);
 
+	/* Clear pending error and receive interrupts */
+	writew(UART011_OEIS | UART011_BEIS | UART011_PEIS | UART011_FEIS |
+	       UART011_RTIS | UART011_RXIS, uap->port.membase + UART011_ICR);
+
 	/*
 	 * Allocate the IRQ
 	 */
@@ -1414,10 +1418,6 @@ static int pl011_startup(struct uart_port *port)
 	cr = UART01x_CR_UARTEN | UART011_CR_RXE | UART011_CR_TXE;
 	writew(cr, uap->port.membase + UART011_CR);
 
-	/* Clear pending error interrupts */
-	writew(UART011_OEIS | UART011_BEIS | UART011_PEIS | UART011_FEIS,
-	       uap->port.membase + UART011_ICR);
-
 	/*
 	 * initialise the old status of the modem signals
 	 */
@@ -1432,6 +1432,9 @@ static int pl011_startup(struct uart_port *port)
 	 * as well.
 	 */
 	spin_lock_irq(&uap->port.lock);
+	/* Clear out any spuriously appearing RX interrupts */
+	 writew(UART011_RTIS | UART011_RXIS,
+		uap->port.membase + UART011_ICR);
 	uap->im = UART011_RTIM;
 	if (!pl011_dma_rx_running(uap))
 		uap->im |= UART011_RXIM;
@@ -1916,6 +1919,10 @@ static int pl011_probe(struct amba_device *dev, const struct amba_id *id)
 		goto unmap;
 	}
 
+	/* Ensure interrupts from this UART are masked and cleared */
+	writew(0, uap->port.membase + UART011_IMSC);
+	writew(0xffff, uap->port.membase + UART011_ICR);
+
 	uap->vendor = vendor;
 	uap->lcrh_rx = vendor->lcrh_rx;
 	uap->lcrh_tx = vendor->lcrh_tx;
-- 
1.7.9.5

