From d8bf8cea10710285b5bc1759162bd18c81d8ea3a Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 25 Jan 2012 12:52:13 +0100
Subject: [PATCH 34/35] beaglebone: really enable i2c2 pullups, fixes timeouts on boot ~4 seconds less wasted

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index 7c91ff8..9556736 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -707,9 +707,9 @@ static struct pinmux_config i2c1_pin_mux[] = {
 
 static struct pinmux_config i2c2_pin_mux[] = {
 	{"uart1_ctsn.i2c2_sda",    OMAP_MUX_MODE3 | AM33XX_SLEWCTRL_SLOW |
-					AM33XX_PULL_ENBL | AM33XX_INPUT_EN},
+					AM33XX_PIN_INPUT_PULLUP},
 	{"uart1_rtsn.i2c2_scl",   OMAP_MUX_MODE3 | AM33XX_SLEWCTRL_SLOW |
-					AM33XX_PULL_ENBL | AM33XX_INPUT_EN},
+					AM33XX_PIN_INPUT_PULLUP},
 	{NULL, 0},
 };
 
-- 
1.7.2.5

