From 375a67105a521c7ae75a529509218c4bda02c612 Mon Sep 17 00:00:00 2001
From: Sarah Sharp <sarah.a.sharp@linux.intel.com>
Date: Fri, 16 Mar 2012 13:27:39 -0700
Subject: [PATCH 37/69] xhci: Restore event ring dequeue pointer on resume.

commit fb3d85bc7193f23c9a564502df95564c49a32c91 upstream.

The xhci_save_registers() function saved the event ring dequeue pointer
in the s3 register structure, but xhci_restore_registers() never
restored it.  No other code in the xHCI successful resume path would
ever restore it either.  Fix that.

This should be backported to kernels as old as 2.6.37, that contain the
commit 5535b1d5f8885695c6ded783c692e3c0d0eda8ca "USB: xHCI: PCI power
management implementation".

Signed-off-by: Sarah Sharp <sarah.a.sharp@linux.intel.com>
Tested-by: Elric Fu <elricfu1@gmail.com>
Cc: Andiry Xu <andiry.xu@amd.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/xhci.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index 034f554..4d44713 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -681,6 +681,7 @@ static void xhci_restore_registers(struct xhci_hcd *xhci)
 	xhci_writel(xhci, xhci->s3.irq_control, &xhci->ir_set->irq_control);
 	xhci_writel(xhci, xhci->s3.erst_size, &xhci->ir_set->erst_size);
 	xhci_write_64(xhci, xhci->s3.erst_base, &xhci->ir_set->erst_base);
+	xhci_write_64(xhci, xhci->s3.erst_dequeue, &xhci->ir_set->erst_dequeue);
 }
 
 static void xhci_set_cmd_ring_deq(struct xhci_hcd *xhci)
-- 
1.7.9.5

