From b69e09a8ee7effdd60a09a38ae8a28c45f000f48 Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Sat, 25 Feb 2012 11:13:16 +0100
Subject: [PATCH 15/95] ALSA: hda/realtek - Fix resume of multiple input
 sources

commit 068b939431486f524438330b0848a8222e33d421 upstream.

When there are multiple input sources, the driver wrongly overwrites with
the value of the last input source on other slots at resume.  Thus the
primary input source may be shown wrongly.

Reported-and-tested-by: Julian Sikorski <belegdol@gmail.com>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/pci/hda/patch_realtek.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/pci/hda/patch_realtek.c b/sound/pci/hda/patch_realtek.c
index c4c8d78..3d8fbf4 100644
--- a/sound/pci/hda/patch_realtek.c
+++ b/sound/pci/hda/patch_realtek.c
@@ -3695,7 +3695,7 @@ static void alc_auto_init_input_src(struct hda_codec *codec)
 	else
 		nums = spec->num_adc_nids;
 	for (c = 0; c < nums; c++)
-		alc_mux_select(codec, 0, spec->cur_mux[c], true);
+		alc_mux_select(codec, c, spec->cur_mux[c], true);
 }
 
 /* add mic boosts if needed */
-- 
1.7.9.4

