From 06c4cfeec98f4f1e31543878ceb74c5fff1907e4 Mon Sep 17 00:00:00 2001
From: Enrico Butera <ebutera@users.berlios.de>
Date: Thu, 22 Dec 2011 11:01:58 +0100
Subject: [PATCH 1/2] adjust videdev headers for recent kernels

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 .../packages/ti/sdo/dmai/linux/omap3530/Capture.c  |    1 -
 .../ti/sdo/dmai/linux/omap3530/Display_v4l2.c      |    1 -
 .../ti/sdo/dmai/linux/omap3530/_VideoBuf.c         |    1 -
 .../ti/sdo/dmai/linux/omap3530/priv/_VideoBuf.h    |    1 -
 4 files changed, 0 insertions(+), 4 deletions(-)

diff --git a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Capture.c b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Capture.c
index a924169..c2b45d2 100644
--- a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Capture.c
+++ b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Capture.c
@@ -40,7 +40,6 @@
 #include <sys/mman.h>
 #include <sys/ioctl.h>
 #include <asm/types.h>
-#include <linux/videodev.h>
 #include <linux/videodev2.h>
 
 #include <xdc/std.h>
diff --git a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Display_v4l2.c b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Display_v4l2.c
index 0d01b39..0c35efe 100644
--- a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Display_v4l2.c
+++ b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/Display_v4l2.c
@@ -38,7 +38,6 @@
 #include <sys/ioctl.h>
 #include <sys/mman.h>
 #include <errno.h>
-#include <linux/videodev.h>
 #include <linux/videodev2.h>
 
 #include <xdc/std.h>
diff --git a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/_VideoBuf.c b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/_VideoBuf.c
index 5615e2f..5cb712d 100644
--- a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/_VideoBuf.c
+++ b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/_VideoBuf.c
@@ -38,7 +38,6 @@
 #include <sys/ioctl.h>
 #include <sys/mman.h>
 #include <errno.h>
-#include <linux/videodev.h>
 #include <linux/videodev2.h>
 
 #include <xdc/std.h>
diff --git a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/priv/_VideoBuf.h b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/priv/_VideoBuf.h
index b2128a3..dbaa4eb 100644
--- a/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/priv/_VideoBuf.h
+++ b/davinci_multimedia_application_interface/dmai/packages/ti/sdo/dmai/linux/omap3530/priv/_VideoBuf.h
@@ -34,7 +34,6 @@
 #ifndef ti_sdo_dai_linux_priv__VideoBuf_h_
 #define ti_sdo_dai_linux_priv__VideoBuf_h_
 
-#include <linux/videodev.h>
 #include <linux/videodev2.h>
 
 #include <ti/sdo/dmai/BufferGfx.h>
-- 
1.7.2.5

