From 9a70f2b5f4dbd354260036f53e4de261a3c127cf Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Mon, 23 Jan 2012 18:23:36 +0100
Subject: [PATCH 02/90] ALSA: hda - Fix silent outputs from docking-station
 jacks of Dell laptops

commit b4ead019afc201f71c39cd0dfcaafed4a97b3dd2 upstream.

The recent change of the power-widget handling for IDT codecs caused
the silent output from the docking-station line-out jack.  This was
partially fixed by the commit f2cbba7602383cd9cdd21f0a5d0b8bd1aad47b33
"ALSA: hda - Fix the lost power-setup of seconary pins after PM resume".
But the line-out on the docking-station is still silent when booted
with the jack plugged even by this fix.

The remainig bug is that the power-widget is set off in stac92xx_init()
because the pins in cfg->line_out_pins[] aren't checked there properly
but only hp_pins[] are checked in is_nid_hp_pin().

This patch fixes the problem by checking both HP and line-out pins
and leaving the power-map correctly.

Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=42637

Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/pci/hda/patch_sigmatel.c |    8 +++++---
 1 file changed, 5 insertions(+), 3 deletions(-)

diff --git a/sound/pci/hda/patch_sigmatel.c b/sound/pci/hda/patch_sigmatel.c
index f3c73a9..2141cab 100644
--- a/sound/pci/hda/patch_sigmatel.c
+++ b/sound/pci/hda/patch_sigmatel.c
@@ -4253,13 +4253,15 @@ static int enable_pin_detect(struct hda_codec *codec, hda_nid_t nid,
 	return 1;
 }
 
-static int is_nid_hp_pin(struct auto_pin_cfg *cfg, hda_nid_t nid)
+static int is_nid_out_jack_pin(struct auto_pin_cfg *cfg, hda_nid_t nid)
 {
 	int i;
 	for (i = 0; i < cfg->hp_outs; i++)
 		if (cfg->hp_pins[i] == nid)
 			return 1; /* nid is a HP-Out */
-
+	for (i = 0; i < cfg->line_outs; i++)
+		if (cfg->line_out_pins[i] == nid)
+			return 1; /* nid is a line-Out */
 	return 0; /* nid is not a HP-Out */
 };
 
@@ -4465,7 +4467,7 @@ static int stac92xx_init(struct hda_codec *codec)
 			continue;
 		}
 
-		if (is_nid_hp_pin(cfg, nid))
+		if (is_nid_out_jack_pin(cfg, nid))
 			continue; /* already has an unsol event */
 
 		pinctl = snd_hda_codec_read(codec, nid, 0,
-- 
1.7.9.4

