From ceaddf58a2932ff4a4dffa216af9db01d1bd74cc Mon Sep 17 00:00:00 2001
From: Rob Clark <rob@ti.com>
Date: Mon, 20 Feb 2012 15:03:36 -0600
Subject: [PATCH 64/95] OMAPDSS: HDMI: hot plug detect fix

commit ca888a7958b3d808e4efd08ceff88913f4212c69 upstream.

The "OMAPDSS: HDMI: PHY burnout fix" commit switched the HDMI driver
over to using a GPIO for plug detect.  Unfortunately the ->detect()
method was not also updated, causing HDMI to no longer work for the
omapdrm driver (because it would actually check if a connection was
detected before attempting to enable display).

Signed-off-by: Rob Clark <rob@ti.com>
Signed-off-by: Tomi Valkeinen <tomi.valkeinen@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/video/omap2/dss/ti_hdmi_4xxx_ip.c |    9 +--------
 1 file changed, 1 insertion(+), 8 deletions(-)

diff --git a/drivers/video/omap2/dss/ti_hdmi_4xxx_ip.c b/drivers/video/omap2/dss/ti_hdmi_4xxx_ip.c
index 3683404..aad48a1 100644
--- a/drivers/video/omap2/dss/ti_hdmi_4xxx_ip.c
+++ b/drivers/video/omap2/dss/ti_hdmi_4xxx_ip.c
@@ -479,14 +479,7 @@ int ti_hdmi_4xxx_read_edid(struct hdmi_ip_data *ip_data,
 
 bool ti_hdmi_4xxx_detect(struct hdmi_ip_data *ip_data)
 {
-	int r;
-
-	void __iomem *base = hdmi_core_sys_base(ip_data);
-
-	/* HPD */
-	r = REG_GET(base, HDMI_CORE_SYS_SYS_STAT, 1, 1);
-
-	return r == 1;
+	return gpio_get_value(ip_data->hpd_gpio);
 }
 
 static void hdmi_core_init(struct hdmi_core_video_config *video_cfg,
-- 
1.7.9.4

