From 461b534b6a695034c7554b2bdf163b2ecb73b80d Mon Sep 17 00:00:00 2001
From: Chris Bagwell <chris@cnpbagwell.com>
Date: Wed, 23 Nov 2011 10:54:27 +0100
Subject: [PATCH 081/130] HID: hid-multitouch - add another eGalax id

commit 1fd8f047490dd0ec4e4db710fcbc1bd4798d944c upstream.

This allows ASUS Eee Slate touchscreens to work.

Signed-off-by: Chris Bagwell <chris@cnpbagwell.com>
Reviewed-by: Benjamin Tissoires <benjamin.tissoires@gmail.com>
Signed-off-by: Jiri Kosina <jkosina@suse.cz>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/hid/hid-core.c       |    1 +
 drivers/hid/hid-ids.h        |    1 +
 drivers/hid/hid-multitouch.c |    3 +++
 3 files changed, 5 insertions(+)

diff --git a/drivers/hid/hid-core.c b/drivers/hid/hid-core.c
index 1473067..b51cbf2 100644
--- a/drivers/hid/hid-core.c
+++ b/drivers/hid/hid-core.c
@@ -1409,6 +1409,7 @@ static const struct hid_device_id hid_have_special_driver[] = {
 	{ HID_USB_DEVICE(USB_VENDOR_ID_DWAV, USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH2) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_DWAV, USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH3) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_DWAV, USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH4) },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_DWAV, USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH5) },
 	{ HID_BLUETOOTH_DEVICE(USB_VENDOR_ID_ELECOM, USB_DEVICE_ID_ELECOM_BM084) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_ELO, USB_DEVICE_ID_ELO_TS2515) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_EMS, USB_DEVICE_ID_EMS_TRIO_LINKER_PLUS_II) },
diff --git a/drivers/hid/hid-ids.h b/drivers/hid/hid-ids.h
index 4a441a6..4c9a342 100644
--- a/drivers/hid/hid-ids.h
+++ b/drivers/hid/hid-ids.h
@@ -235,6 +235,7 @@
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH2	0x72a1
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH3	0x480e
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH4	0x726b
+#define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH5	0xa001
 
 #define USB_VENDOR_ID_ELECOM		0x056e
 #define USB_DEVICE_ID_ELECOM_BM084	0x0061
diff --git a/drivers/hid/hid-multitouch.c b/drivers/hid/hid-multitouch.c
index f1c909f..a59d939 100644
--- a/drivers/hid/hid-multitouch.c
+++ b/drivers/hid/hid-multitouch.c
@@ -662,6 +662,9 @@ static const struct hid_device_id mt_devices[] = {
 	{  .driver_data = MT_CLS_EGALAX,
 		HID_USB_DEVICE(USB_VENDOR_ID_DWAV,
 			USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH4) },
+	{  .driver_data = MT_CLS_EGALAX,
+		HID_USB_DEVICE(USB_VENDOR_ID_DWAV,
+			USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH5) },
 
 	/* Elo TouchSystems IntelliTouch Plus panel */
 	{ .driver_data = MT_CLS_DUAL_NSMU_CONTACTID,
-- 
1.7.9.4

