From 2a2a58328a4241c30b0464b700899e7ba93a10a1 Mon Sep 17 00:00:00 2001
From: Mark Brown <broonie@opensource.wolfsonmicro.com>
Date: Wed, 22 Feb 2012 15:52:56 +0000
Subject: [PATCH 45/95] ASoC: dapm: Check for bias level when powering down

commit 7679e42ec833ed70aa34790a5f39dcb7e5bda4fe upstream.

Recent enhancements in the bias management means that we might not be
in standby when the CODEC is idle and can have active widgets without
being in full power mode but the shutdown functionality assumes these
things. Add checks for the bias level at each stage so that we don't
do transitions other than the ON->PREPARE->STANDBY->OFF ones that the
drivers are expecting.

Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/soc-dapm.c |   12 +++++++++---
 1 file changed, 9 insertions(+), 3 deletions(-)

diff --git a/sound/soc/soc-dapm.c b/sound/soc/soc-dapm.c
index f42e8b9..ea909c5 100644
--- a/sound/soc/soc-dapm.c
+++ b/sound/soc/soc-dapm.c
@@ -2982,9 +2982,13 @@ static void soc_dapm_shutdown_codec(struct snd_soc_dapm_context *dapm)
 	 * standby.
 	 */
 	if (powerdown) {
-		snd_soc_dapm_set_bias_level(dapm, SND_SOC_BIAS_PREPARE);
+		if (dapm->bias_level == SND_SOC_BIAS_ON)
+			snd_soc_dapm_set_bias_level(dapm,
+						    SND_SOC_BIAS_PREPARE);
 		dapm_seq_run(dapm, &down_list, 0, false);
-		snd_soc_dapm_set_bias_level(dapm, SND_SOC_BIAS_STANDBY);
+		if (dapm->bias_level == SND_SOC_BIAS_PREPARE)
+			snd_soc_dapm_set_bias_level(dapm,
+						    SND_SOC_BIAS_STANDBY);
 	}
 }
 
@@ -2997,7 +3001,9 @@ void snd_soc_dapm_shutdown(struct snd_soc_card *card)
 
 	list_for_each_entry(codec, &card->codec_dev_list, list) {
 		soc_dapm_shutdown_codec(&codec->dapm);
-		snd_soc_dapm_set_bias_level(&codec->dapm, SND_SOC_BIAS_OFF);
+		if (codec->dapm.bias_level == SND_SOC_BIAS_STANDBY)
+			snd_soc_dapm_set_bias_level(&codec->dapm,
+						    SND_SOC_BIAS_OFF);
 	}
 }
 
-- 
1.7.9.4

