From 4089ed795fc26961e0e0ece07af2c628b96321de Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 25 Jan 2012 17:18:43 +0100
Subject: [PATCH 36/36] beaglebone: update LCD cape partnumber

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index 1b398c7..6a0ace9 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -1356,7 +1356,7 @@ static void beaglebone_cape_setup(struct memory_accessor *mem_acc, void *context
 			pr_info("BeagleBone cape: initializing DVI cape\n");
 			dvi_init(0,0);
 	}
-	if (!strncmp("LCD01", cape_config.partnumber, 5)) {
+	if (!strncmp("BB-BONE-LCD7-01", cape_config.partnumber, 5)) {
 		pr_info("BeagleBone cape: initializing LCD cape\n");
 		bbtoys7lcd_init(0,0);
 		pr_info("BeagleBone cape: initializing LCD cape touchscreen\n");
-- 
1.7.7.5

