From 9bd4b771e9f598f5cebad5146585eb30ececf118 Mon Sep 17 00:00:00 2001
From: Benjamin Tissoires <benjamin.tissoires@enac.fr>
Date: Wed, 23 Nov 2011 10:54:33 +0100
Subject: [PATCH 084/130] HID: multitouch: add support for the MSI Windpad
 110W

commit 66f06127f34ad6e8a1b24a2c03144b694d19f99f upstream.

Just another eGalax device.
Please note that adding this device to have_special_driver
in hid-core.c is not required anymore.

Signed-off-by: Benjamin Tissoires <benjamin.tissoires@enac.fr>
Signed-off-by: Jiri Kosina <jkosina@suse.cz>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/hid/hid-ids.h        |    1 +
 drivers/hid/hid-multitouch.c |    3 +++
 2 files changed, 4 insertions(+)

diff --git a/drivers/hid/hid-ids.h b/drivers/hid/hid-ids.h
index 9eb90b1..6ccd7df 100644
--- a/drivers/hid/hid-ids.h
+++ b/drivers/hid/hid-ids.h
@@ -235,6 +235,7 @@
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_720C	0x720c
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_726B	0x726b
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_72A1	0x72a1
+#define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_72FA	0x72fa
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_7302	0x7302
 #define USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_A001	0xa001
 
diff --git a/drivers/hid/hid-multitouch.c b/drivers/hid/hid-multitouch.c
index c77d495..6f6b1d9 100644
--- a/drivers/hid/hid-multitouch.c
+++ b/drivers/hid/hid-multitouch.c
@@ -664,6 +664,9 @@ static const struct hid_device_id mt_devices[] = {
 			USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_72A1) },
 	{ .driver_data = MT_CLS_EGALAX,
 		HID_USB_DEVICE(USB_VENDOR_ID_DWAV,
+			USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_72FA) },
+	{ .driver_data = MT_CLS_EGALAX,
+		HID_USB_DEVICE(USB_VENDOR_ID_DWAV,
 			USB_DEVICE_ID_DWAV_EGALAX_MULTITOUCH_7302) },
 	{ .driver_data = MT_CLS_EGALAX,
 		HID_USB_DEVICE(USB_VENDOR_ID_DWAV,
-- 
1.7.9.4

