From b140872c2b68584d6222963186857872b0b4aad8 Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Tue, 24 Jan 2012 13:58:36 +0100
Subject: [PATCH 02/87] ALSA: hda - Fix the logic to detect VIA analog
 low-current mode

commit 924339239fd5ba3e505f9420d41f0939196f3530 upstream.

The analog low-current mode must be enabled when the no stream is
running but the current detection checks it in a wrong way.

Bugzilla: https://bugzilla.novell.com/show_bug.cgi?id=741128

Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/pci/hda/patch_via.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/pci/hda/patch_via.c b/sound/pci/hda/patch_via.c
index 8d69e59..0684542 100644
--- a/sound/pci/hda/patch_via.c
+++ b/sound/pci/hda/patch_via.c
@@ -1041,7 +1041,7 @@ static void analog_low_current_mode(struct hda_codec *codec)
 	bool enable;
 	unsigned int verb, parm;
 
-	enable = is_aa_path_mute(codec) && (spec->opened_streams != 0);
+	enable = is_aa_path_mute(codec) && !spec->opened_streams;
 
 	/* decide low current mode's verb & parameter */
 	switch (spec->codec_type) {
-- 
1.7.9.4

