From 9f3da92a62f59784ea39eaa38e259f0185bd5d09 Mon Sep 17 00:00:00 2001
From: Claudio Scordino <claudio@evidence.eu.com>
Date: Fri, 16 Dec 2011 15:08:49 +0100
Subject: [PATCH 30/49] atmel_serial: fix spinlock lockup in RS485 code

commit dbf1115d3f8c7052788aa4e6e46abd27f3b3eeba upstream.

Patch to fix a spinlock lockup in the driver that sometimes happens when the
tasklet starts.

Signed-off-by: Claudio Scordino <claudio@evidence.eu.com>
Signed-off-by: Dave Bender <codehero@gmail.com>
Tested-by: Dave Bender <codehero@gmail.com>
Acked-by: Nicolas Ferre <nicolas.ferre@atmel.com>
Acked-by: Alan Cox <alan@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/tty/serial/atmel_serial.c |    5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

diff --git a/drivers/tty/serial/atmel_serial.c b/drivers/tty/serial/atmel_serial.c
index 4c823f3..90c8e3a 100644
--- a/drivers/tty/serial/atmel_serial.c
+++ b/drivers/tty/serial/atmel_serial.c
@@ -212,8 +212,9 @@ void atmel_config_rs485(struct uart_port *port, struct serial_rs485 *rs485conf)
 {
 	struct atmel_uart_port *atmel_port = to_atmel_uart_port(port);
 	unsigned int mode;
+	unsigned long flags;
 
-	spin_lock(&port->lock);
+	spin_lock_irqsave(&port->lock, flags);
 
 	/* Disable interrupts */
 	UART_PUT_IDR(port, atmel_port->tx_done_mask);
@@ -244,7 +245,7 @@ void atmel_config_rs485(struct uart_port *port, struct serial_rs485 *rs485conf)
 	/* Enable interrupts */
 	UART_PUT_IER(port, atmel_port->tx_done_mask);
 
-	spin_unlock(&port->lock);
+	spin_unlock_irqrestore(&port->lock, flags);
 
 }
 
-- 
1.7.9.4

