From b744cbb89e3dd00a3f12d349ec0be604dffb5776 Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Thu, 24 Jun 2010 16:34:13 -0500
Subject: [PATCH 20/75] omap3beagle: camera: set mclk for mt9t111

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 arch/arm/mach-omap2/board-omap3beagle-camera.c |    5 +++++
 1 files changed, 5 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle-camera.c b/arch/arm/mach-omap2/board-omap3beagle-camera.c
index 75c8345..529a6be 100644
--- a/arch/arm/mach-omap2/board-omap3beagle-camera.c
+++ b/arch/arm/mach-omap2/board-omap3beagle-camera.c
@@ -49,6 +49,8 @@
 
 #define CAM_USE_XCLKA       0
 
+#define ISP_MT9T111_MCLK		216000000
+
 static struct regulator *beagle_mt9t111_reg1;
 static struct regulator *beagle_mt9t111_reg2;
 
@@ -60,6 +62,9 @@ static struct isp_interface_config mt9t111_if_config = {
 	.strobe			= 0x0,
 	.prestrobe		= 0x0,
 	.shutter		= 0x0,
+	.cam_mclk		= ISP_MT9T111_MCLK,
+	.wenlog 		= ISPCCDC_CFG_WENLOG_AND,
+	.wait_hs_vs		= 2,
 	.u.par.par_bridge	= 0x1,
 	.u.par.par_clk_pol	= 0x0,
 };
-- 
1.6.6.1

